<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="22" y2="0" width="0" layer="20"/>
<wire x1="22" y1="0" x2="22" y2="17" width="0" layer="20"/>
<wire x1="22" y1="17" x2="0" y2="17" width="0" layer="20"/>
<wire x1="0" y1="17" x2="0" y2="0" width="0" layer="20"/>
<text>POKEY/SIDMAX
JTAG adaptor</text>
</plain>
<libraries>
<library name="con-headers-jp">
<description>&lt;b&gt;Male(J), Female(P) and Pin Headers&lt;/b&gt;&lt;p&gt;Version 1.02 - 03/10/2009&lt;p&gt;
This library is a collection of various pin headers and AMP, Molex and 3M board-to-board connectors. 
This library assumes the notion of JACKS(male) and PLUGS(female) as represented by the J and P symbols.
Standard male/female pin header types are available in common 0.1" and 2 mm pitch types with alternate mirrored footprints as well.
&lt;p&gt;THIS LIBRARY IS PROVIDED AS IS AND WITHOUT WARRANTY OF ANY KIND, EXPRESSED OR IMPLIED.&lt;br&gt;
USE AT YOUR OWN RISK!&lt;p&gt;
&lt;author&gt;Copyright (C) 2008, Bob Starr&lt;br&gt; http://www.bobstarr.net&lt;br&gt;&lt;/author&gt;</description>
<packages>
<package name="DIL-100-2X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt; - 0.1"</description>
</package>
</packages>
</library>
<library name="con-ml">
<packages>
<package name="ML10">
<description>&lt;b&gt;HARTING&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="P2" library="con-headers-jp" package="DIL-100-2X03" value="M-2X03-DIL-100">
<attribute name="VALUE"/>
</element>
<element name="SV1" library="con-ml" package="ML10" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="TCK">
<contactref element="P2" pad="4"/>
<contactref element="SV1" pad="1"/>
</signal>
<signal name="TDO">
<contactref element="P2" pad="6"/>
<contactref element="SV1" pad="3"/>
</signal>
<signal name="TMS">
<contactref element="P2" pad="1"/>
<contactref element="SV1" pad="5"/>
</signal>
<signal name="TDI">
<contactref element="P2" pad="3"/>
<contactref element="SV1" pad="9"/>
</signal>
<signal name="GND">
<contactref element="P2" pad="5"/>
<contactref element="SV1" pad="2"/>
</signal>
<signal name="3V3">
<contactref element="P2" pad="2"/>
<contactref element="SV1" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
