<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<text>éclaire XL
The Complete 8-bit   Hardware
(c)2016 by Mark Watson
PCB Reroute by Panos Santos
Thanks to Matthias Reichl
Version 1.0</text>
<text>8-bit
V DAC</text>
<text>10-bit
 A/DC</text>
<text>V G A</text>
<wire x1="170" y1="0.8" x2="170" y2="169.365" width="0.254" layer="20"/>
<wire x1="170" y1="169.365" x2="169.365" y2="170" width="0.254" layer="20" curve="90"/>
<wire x1="169.365" y1="170" x2="0.635" y2="170" width="0.254" layer="20"/>
<wire x1="0.635" y1="170" x2="0" y2="169.365" width="0.254" layer="20" curve="90"/>
<wire x1="0" y1="169.365" x2="0" y2="0.635" width="0.254" layer="20"/>
<wire x1="0" y1="0.635" x2="0.635" y2="0" width="0.254" layer="20" curve="90"/>
<wire x1="0.635" y1="0" x2="169.3672" y2="0" width="0.254" layer="20"/>
<wire x1="169.3672" y1="0" x2="170.0022" y2="0.635" width="0.254" layer="20" curve="90"/>
<wire x1="170.0022" y1="0.635" x2="170.0022" y2="0.9144" width="0.254" layer="20"/>
<text>1-2 COMP</text>
<text>2-3 S-VIDEO</text>
<text>Delta Sigma Audio Filter</text>
<text>+</text>
<text>-</text>
<text>REGULATION</text>
<text>DECOUPLING!!</text>
<text>1</text>
<text>QS3384</text>
<text>QS3384</text>
<text>QS3384</text>
<text>QS3384</text>
<text>CARTRIDGE / P.B.I.</text>
<text>INTERFACE</text>
<text>1</text>
<text>1</text>
<text>éclaire XL
The Complete 8-bit   Hardware
(c)2016 by Mark Watson
PCB Reroute by Panos Santos
Thanks to Matthias Reichl
Version 1.0</text>
<text>USB A</text>
<text>USB B</text>
<text>AUDIO </text>
<text>RS232 PORT</text>
<text>QS3384</text>
<text>P
O
W
E
R

G
O
O
D</text>
<text>P
O
W
E
R

G
O
O
D</text>
<text>TEST POINTS!!</text>
<text>3v3</text>
<text>2v5</text>
<text>1v1</text>
<text>GND</text>
<text>1. TO AC97
2. TO SIO
3. TO PBI</text>
<text>V G A</text>
<text>HDMI</text>
<text>LED</text>
<text>K</text>
<text>K</text>
<text>K</text>
</plain>
<libraries>
<library name="rcl">
<description>&lt;b&gt;Resistors, Capacitors, Inductors&lt;/b&gt;&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;r.lbr
&lt;li&gt;cap.lbr 
&lt;li&gt;cap-fe.lbr
&lt;li&gt;captant.lbr
&lt;li&gt;polcap.lbr
&lt;li&gt;ipc-smd.lbr
&lt;/ul&gt;
All SMD packages are defined according to the IPC specifications and  CECC&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
for Electrolyt Capacitors see also :&lt;p&gt;
www.bccomponents.com &lt;p&gt;
www.panasonic.com&lt;p&gt;
www.kemet.com&lt;p&gt;
http://www.secc.co.jp/pdf/os_e/2004/e_os_all.pdf &lt;b&gt;(SANYO)&lt;/b&gt;
&lt;p&gt;
for trimmer refence see : &lt;u&gt;www.electrospec-inc.com/cross_references/trimpotcrossref.asp&lt;/u&gt;&lt;p&gt;

&lt;table border=0 cellspacing=0 cellpadding=0 width="100%" cellpaddding=0&gt;
&lt;tr valign="top"&gt;

&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;TRIM-POT CROSS REFERENCE&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;RECTANGULAR MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BOURNS&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BI&amp;nbsp;TECH&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;DALE-VISHAY&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PHILIPS/MEPCO&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MURATA&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PANASONIC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;SPECTROL&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MILSPEC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;&lt;TD&gt;&amp;nbsp;&lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3 &gt;
      3005P&lt;BR&gt;
      3006P&lt;BR&gt;
      3006W&lt;BR&gt;
      3006Y&lt;BR&gt;
      3009P&lt;BR&gt;
      3009W&lt;BR&gt;
      3009Y&lt;BR&gt;
      3057J&lt;BR&gt;
      3057L&lt;BR&gt;
      3057P&lt;BR&gt;
      3057Y&lt;BR&gt;
      3059J&lt;BR&gt;
      3059L&lt;BR&gt;
      3059P&lt;BR&gt;
      3059Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      89P&lt;BR&gt;
      89W&lt;BR&gt;
      89X&lt;BR&gt;
      89PH&lt;BR&gt;
      76P&lt;BR&gt;
      89XH&lt;BR&gt;
      78SLT&lt;BR&gt;
      78L&amp;nbsp;ALT&lt;BR&gt;
      56P&amp;nbsp;ALT&lt;BR&gt;
      78P&amp;nbsp;ALT&lt;BR&gt;
      T8S&lt;BR&gt;
      78L&lt;BR&gt;
      56P&lt;BR&gt;
      78P&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      T18/784&lt;BR&gt;
      783&lt;BR&gt;
      781&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2199&lt;BR&gt;
      1697/1897&lt;BR&gt;
      1680/1880&lt;BR&gt;
      2187&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      8035EKP/CT20/RJ-20P&lt;BR&gt;
      -&lt;BR&gt;
      RJ-20X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      1211L&lt;BR&gt;
      8012EKQ&amp;nbsp;ALT&lt;BR&gt;
      8012EKR&amp;nbsp;ALT&lt;BR&gt;
      1211P&lt;BR&gt;
      8012EKJ&lt;BR&gt;
      8012EKL&lt;BR&gt;
      8012EKQ&lt;BR&gt;
      8012EKR&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      2101P&lt;BR&gt;
      2101W&lt;BR&gt;
      2101Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2102L&lt;BR&gt;
      2102S&lt;BR&gt;
      2102Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVMCOG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      43P&lt;BR&gt;
      43W&lt;BR&gt;
      43Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      40L&lt;BR&gt;
      40P&lt;BR&gt;
      40Y&lt;BR&gt;
      70Y-T602&lt;BR&gt;
      70L&lt;BR&gt;
      70P&lt;BR&gt;
      70Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SQUARE MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
   &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3250L&lt;BR&gt;
      3250P&lt;BR&gt;
      3250W&lt;BR&gt;
      3250X&lt;BR&gt;
      3252P&lt;BR&gt;
      3252W&lt;BR&gt;
      3252X&lt;BR&gt;
      3260P&lt;BR&gt;
      3260W&lt;BR&gt;
      3260X&lt;BR&gt;
      3262P&lt;BR&gt;
      3262W&lt;BR&gt;
      3262X&lt;BR&gt;
      3266P&lt;BR&gt;
      3266W&lt;BR&gt;
      3266X&lt;BR&gt;
      3290H&lt;BR&gt;
      3290P&lt;BR&gt;
      3290W&lt;BR&gt;
      3292P&lt;BR&gt;
      3292W&lt;BR&gt;
      3292X&lt;BR&gt;
      3296P&lt;BR&gt;
      3296W&lt;BR&gt;
      3296X&lt;BR&gt;
      3296Y&lt;BR&gt;
      3296Z&lt;BR&gt;
      3299P&lt;BR&gt;
      3299W&lt;BR&gt;
      3299X&lt;BR&gt;
      3299Y&lt;BR&gt;
      3299Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64P&amp;nbsp;ALT&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      64X&amp;nbsp;ALT&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66P&lt;BR&gt;
      66W&lt;BR&gt;
      66X&lt;BR&gt;
      67P&lt;BR&gt;
      67W&lt;BR&gt;
      67X&lt;BR&gt;
      67Y&lt;BR&gt;
      67Z&lt;BR&gt;
      68P&lt;BR&gt;
      68W&lt;BR&gt;
      68X&lt;BR&gt;
      67Y&amp;nbsp;ALT&lt;BR&gt;
      67Z&amp;nbsp;ALT&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      5050&lt;BR&gt;
      5091&lt;BR&gt;
      5080&lt;BR&gt;
      5087&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T63YB&lt;BR&gt;
      T63XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      5887&lt;BR&gt;
      5891&lt;BR&gt;
      5880&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T93Z&lt;BR&gt;
      T93YA&lt;BR&gt;
      T93XA&lt;BR&gt;
      T93YB&lt;BR&gt;
      T93XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKW&lt;BR&gt;
      8026EKM&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKB&lt;BR&gt;
      8026EKM&lt;BR&gt;
      1309X&lt;BR&gt;
      1309P&lt;BR&gt;
      1309W&lt;BR&gt;
      8024EKP&lt;BR&gt;
      8024EKW&lt;BR&gt;
      8024EKN&lt;BR&gt;
      RJ-9P/CT9P&lt;BR&gt;
      RJ-9W&lt;BR&gt;
      RJ-9X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3105P/3106P&lt;BR&gt;
      3105W/3106W&lt;BR&gt;
      3105X/3106X&lt;BR&gt;
      3105Y/3106Y&lt;BR&gt;
      3105Z/3105Z&lt;BR&gt;
      3102P&lt;BR&gt;
      3102W&lt;BR&gt;
      3102X&lt;BR&gt;
      3102Y&lt;BR&gt;
      3102Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMCBG&lt;BR&gt;
      EVMCCG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      55-1-X&lt;BR&gt;
      55-4-X&lt;BR&gt;
      55-3-X&lt;BR&gt;
      55-2-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      50-2-X&lt;BR&gt;
      50-4-X&lt;BR&gt;
      50-3-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      64Y&lt;BR&gt;
      64Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3323P&lt;BR&gt;
      3323S&lt;BR&gt;
      3323W&lt;BR&gt;
      3329H&lt;BR&gt;
      3329P&lt;BR&gt;
      3329W&lt;BR&gt;
      3339H&lt;BR&gt;
      3339P&lt;BR&gt;
      3339W&lt;BR&gt;
      3352E&lt;BR&gt;
      3352H&lt;BR&gt;
      3352K&lt;BR&gt;
      3352P&lt;BR&gt;
      3352T&lt;BR&gt;
      3352V&lt;BR&gt;
      3352W&lt;BR&gt;
      3362H&lt;BR&gt;
      3362M&lt;BR&gt;
      3362P&lt;BR&gt;
      3362R&lt;BR&gt;
      3362S&lt;BR&gt;
      3362U&lt;BR&gt;
      3362W&lt;BR&gt;
      3362X&lt;BR&gt;
      3386B&lt;BR&gt;
      3386C&lt;BR&gt;
      3386F&lt;BR&gt;
      3386H&lt;BR&gt;
      3386K&lt;BR&gt;
      3386M&lt;BR&gt;
      3386P&lt;BR&gt;
      3386S&lt;BR&gt;
      3386W&lt;BR&gt;
      3386X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      25P&lt;BR&gt;
      25S&lt;BR&gt;
      25RX&lt;BR&gt;
      82P&lt;BR&gt;
      82M&lt;BR&gt;
      82PA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      91E&lt;BR&gt;
      91X&lt;BR&gt;
      91T&lt;BR&gt;
      91B&lt;BR&gt;
      91A&lt;BR&gt;
      91V&lt;BR&gt;
      91W&lt;BR&gt;
      25W&lt;BR&gt;
      25V&lt;BR&gt;
      25P&lt;BR&gt;
      -&lt;BR&gt;
      25S&lt;BR&gt;
      25U&lt;BR&gt;
      25RX&lt;BR&gt;
      25X&lt;BR&gt;
      72XW&lt;BR&gt;
      72XL&lt;BR&gt;
      72PM&lt;BR&gt;
      72RX&lt;BR&gt;
      -&lt;BR&gt;
      72PX&lt;BR&gt;
      72P&lt;BR&gt;
      72RXW&lt;BR&gt;
      72RXL&lt;BR&gt;
      72X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T7YB&lt;BR&gt;
      T7YA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      TXD&lt;BR&gt;
      TYA&lt;BR&gt;
      TYP&lt;BR&gt;
      -&lt;BR&gt;
      TYD&lt;BR&gt;
      TX&lt;BR&gt;
      -&lt;BR&gt;
      150SX&lt;BR&gt;
      100SX&lt;BR&gt;
      102T&lt;BR&gt;
      101S&lt;BR&gt;
      190T&lt;BR&gt;
      150TX&lt;BR&gt;
      101&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      101SX&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ET6P&lt;BR&gt;
      ET6S&lt;BR&gt;
      ET6X&lt;BR&gt;
      RJ-6W/8014EMW&lt;BR&gt;
      RJ-6P/8014EMP&lt;BR&gt;
      RJ-6X/8014EMX&lt;BR&gt;
      TM7W&lt;BR&gt;
      TM7P&lt;BR&gt;
      TM7X&lt;BR&gt;
      -&lt;BR&gt;
      8017SMS&lt;BR&gt;
      -&lt;BR&gt;
      8017SMB&lt;BR&gt;
      8017SMA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      CT-6W&lt;BR&gt;
      CT-6H&lt;BR&gt;
      CT-6P&lt;BR&gt;
      CT-6R&lt;BR&gt;
      -&lt;BR&gt;
      CT-6V&lt;BR&gt;
      CT-6X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKV&lt;BR&gt;
      -&lt;BR&gt;
      8038EKX&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKP&lt;BR&gt;
      8038EKZ&lt;BR&gt;
      8038EKW&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3321H&lt;BR&gt;
      3321P&lt;BR&gt;
      3321N&lt;BR&gt;
      1102H&lt;BR&gt;
      1102P&lt;BR&gt;
      1102T&lt;BR&gt;
      RVA0911V304A&lt;BR&gt;
      -&lt;BR&gt;
      RVA0911H413A&lt;BR&gt;
      RVG0707V100A&lt;BR&gt;
      RVA0607V(H)306A&lt;BR&gt;
      RVA1214H213A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3104B&lt;BR&gt;
      3104C&lt;BR&gt;
      3104F&lt;BR&gt;
      3104H&lt;BR&gt;
      -&lt;BR&gt;
      3104M&lt;BR&gt;
      3104P&lt;BR&gt;
      3104S&lt;BR&gt;
      3104W&lt;BR&gt;
      3104X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      EVMQ0G&lt;BR&gt;
      EVMQIG&lt;BR&gt;
      EVMQ3G&lt;BR&gt;
      EVMS0G&lt;BR&gt;
      EVMQ0G&lt;BR&gt;
      EVMG0G&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMK4GA00B&lt;BR&gt;
      EVM30GA00B&lt;BR&gt;
      EVMK0GA00B&lt;BR&gt;
      EVM38GA00B&lt;BR&gt;
      EVMB6&lt;BR&gt;
      EVLQ0&lt;BR&gt;
      -&lt;BR&gt;
      EVMMSG&lt;BR&gt;
      EVMMBG&lt;BR&gt;
      EVMMAG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMMCS&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM0&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM3&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      62-3-1&lt;BR&gt;
      62-1-2&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67R&lt;BR&gt;
      -&lt;BR&gt;
      67P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67X&lt;BR&gt;
      63V&lt;BR&gt;
      63S&lt;BR&gt;
      63M&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63H&lt;BR&gt;
      63P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;&amp;nbsp;&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=3&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT color="#0000FF" SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SMD TRIM-POT CROSS REFERENCE&lt;/B&gt;&lt;/FONT&gt;
      &lt;P&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3224G&lt;BR&gt;
      3224J&lt;BR&gt;
      3224W&lt;BR&gt;
      3269P&lt;BR&gt;
      3269W&lt;BR&gt;
      3269X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      44G&lt;BR&gt;
      44J&lt;BR&gt;
      44W&lt;BR&gt;
      84P&lt;BR&gt;
      84W&lt;BR&gt;
      84X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST63Z&lt;BR&gt;
      ST63Y&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST5P&lt;BR&gt;
      ST5W&lt;BR&gt;
      ST5X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3314G&lt;BR&gt;
      3314J&lt;BR&gt;
      3364A/B&lt;BR&gt;
      3364C/D&lt;BR&gt;
      3364W/X&lt;BR&gt;
      3313G&lt;BR&gt;
      3313J&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      23B&lt;BR&gt;
      23A&lt;BR&gt;
      21X&lt;BR&gt;
      21W&lt;BR&gt;
      -&lt;BR&gt;
      22B&lt;BR&gt;
      22A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST5YL/ST53YL&lt;BR&gt;
      ST5YJ/5T53YJ&lt;BR&gt;
      ST-23A&lt;BR&gt;
      ST-22B&lt;BR&gt;
      ST-22&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST-4B&lt;BR&gt;
      ST-4A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST-3B&lt;BR&gt;
      ST-3A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVM-6YS&lt;BR&gt;
      EVM-1E&lt;BR&gt;
      EVM-1G&lt;BR&gt;
      EVM-1D&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      G4B&lt;BR&gt;
      G4A&lt;BR&gt;
      TR04-3S1&lt;BR&gt;
      TRG04-2S1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      DVR-43A&lt;BR&gt;
      CVR-42C&lt;BR&gt;
      CVR-42A/C&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;
&lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;ALT =&amp;nbsp;ALTERNATE&lt;/B&gt;&lt;/FONT&gt;
&lt;P&gt;

&amp;nbsp;
&lt;P&gt;
&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;</description>
<packages>
<package name="M0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.10 W</description>
</package>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="L3225M">
<description>&lt;b&gt;INDUCTOR&lt;/b&gt;&lt;p&gt;
molded</description>
</package>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="crystal">
<description>&lt;b&gt;Crystals and Crystal Resonators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SG-636">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DB15">
</package>
</packages>
</library>
<library name="Analog Devices_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 31/07/2012 09:37:13</description>
<packages>
<package name="QFP50P900X900X120-49N">
</package>
</packages>
</library>
<library name="con-yamaichi">
<description>&lt;b&gt;Yamaichi Connectors&lt;/b&gt;&lt;p&gt;
Mini-DIN, USB, Fire Wire&lt;br&gt;
DIN female/male, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MDIN04SS">
<description>&lt;b&gt;Mini Din&lt;/b&gt; YAMAICHI CONNECTOR</description>
</package>
</packages>
</library>
<library name="resistor-array">
<description>&lt;b&gt;SMD Resistor Arrays&lt;/b&gt;&lt;p&gt;
CTS, Rohm, etc&lt;p&gt;
&lt;p&gt;THIS LIBRARY IS PROVIDED AS IS AND WITHOUT WARRANTY OF ANY KIND, EXPRESSED OR IMPLIED.&lt;br&gt;
USE AT YOUR OWN RISK!&lt;p&gt;
&lt;author&gt;Copyright (C) 2008, Bob Starr&lt;br&gt; http://www.bobstarr.net&lt;br&gt;&lt;/author&gt;</description>
<packages>
<package name="743-8">
<description>CTS 744 Series&lt;p&gt;
8 Terminations, 4 Resistors</description>
</package>
</packages>
</library>
<library name="sdram">
<description>&lt;b&gt;SDRAM  memories&lt;/b&gt;

by Martin Hinner&lt;br&gt;
&lt;a href="http://martin.hinner.info/"&gt;http://martin.hinner.info/&lt;/a&gt;</description>
<packages>
<package name="TSOP54">
<description>TSOP 54 Pin, pitch 0.8 mm</description>
</package>
</packages>
</library>
<library name="Exar_By_element14_Batch_1">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 30/07/2012 17:16:13</description>
<packages>
<package name="SOT95P280X145-5N">
</package>
</packages>
</library>
<library name="cyclonev_f484">
<packages>
<package name="CYCLONEVF484V2">
</package>
</packages>
</library>
<library name="adc">
<packages>
<package name="SOT95P280X145-5N">
</package>
</packages>
</library>
<library name="header127">
<packages>
<package name="HDR_141_36">
</package>
</packages>
</library>
<library name="epcs">
<packages>
<package name="EPCS_BOTH">
</package>
</packages>
</library>
<library name="raspberrypi_cm">
<packages>
<package name="HDMI">
</package>
</packages>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="JP2">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
</package>
<package name="JP1">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
</package>
<package name="JP3Q">
<description>&lt;b&gt;JUMPER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,6-PAD">
<description>&lt;b&gt;MOUNTING PAD&lt;/b&gt; 3.6 mm, round</description>
</package>
</packages>
</library>
<library name="molex_ps">
<packages>
<package name="MOLEX_PS">
</package>
</packages>
</library>
<library name="con-subd">
<description>&lt;b&gt;SUB-D Connectors&lt;/b&gt;&lt;p&gt;
Harting&lt;br&gt;
NorComp&lt;br&gt;
&lt;p&gt;
PREFIX :&lt;br&gt;
H = High density&lt;br&gt;
F = Female&lt;br&gt;
M = Male&lt;p&gt;
NUMBER: Number of pins&lt;p&gt;
SUFFIX :&lt;br&gt;
H = Horizontal&lt;br&gt;
V = Vertical &lt;br&gt;
P = Shield pin on housing&lt;br&gt;
B = No mounting holes&lt;br&gt;
S = Pins individually placeable (Single)&lt;br&gt;
D = Direct mounting &lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="M09HP">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
<package name="F09V">
<description>&lt;b&gt;SUB-D&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="transistor-pnp">
<description>&lt;b&gt;PNP Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23-BEC">
<description>&lt;b&gt;TO-236&lt;/b&gt; ITT Intermetall</description>
</package>
</packages>
</library>
<library name="quickswitch">
<packages>
<package name="TSSOP24">
<description>&lt;b&gt;Thin Shrink Small Outline Plastic 24&lt;/b&gt;&lt;p&gt;
MAX3223-MAX3243.pdf</description>
</package>
<package name="SOD123">
<description>&lt;b&gt;SMALL OUTLINE DIODE&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="resistor">
<description>&lt;b&gt;Resistors, Capacitors, Inductors&lt;/b&gt;&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;r.lbr
&lt;li&gt;cap.lbr 
&lt;li&gt;cap-fe.lbr
&lt;li&gt;captant.lbr
&lt;li&gt;polcap.lbr
&lt;li&gt;ipc-smd.lbr
&lt;/ul&gt;
All SMD packages are defined according to the IPC specifications and  CECC&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
for Electrolyt Capacitors see also :&lt;p&gt;
www.bccomponents.com &lt;p&gt;
www.panasonic.com&lt;p&gt;
www.kemet.com&lt;p&gt;
&lt;p&gt;
for trimmer refence see : &lt;u&gt;www.electrospec-inc.com/cross_references/trimpotcrossref.asp&lt;/u&gt;&lt;p&gt;

&lt;map name="nav_main"&gt;
&lt;area shape="rect" coords="0,1,140,23" href="../military_specs.asp" title=""&gt;
&lt;area shape="rect" coords="0,24,140,51" href="../about.asp" title=""&gt;
&lt;area shape="rect" coords="1,52,140,77" href="../rfq.asp" title=""&gt;
&lt;area shape="rect" coords="0,78,139,103" href="../products.asp" title=""&gt;
&lt;area shape="rect" coords="1,102,138,128" href="../excess_inventory.asp" title=""&gt;
&lt;area shape="rect" coords="1,129,138,150" href="../edge.asp" title=""&gt;
&lt;area shape="rect" coords="1,151,139,178" href="../industry_links.asp" title=""&gt;
&lt;area shape="rect" coords="0,179,139,201" href="../comments.asp" title=""&gt;
&lt;area shape="rect" coords="1,203,138,231" href="../directory.asp" title=""&gt;
&lt;area shape="default" nohref&gt;
&lt;/map&gt;

&lt;html&gt;

&lt;title&gt;&lt;/title&gt;

 &lt;LINK REL="StyleSheet" TYPE="text/css" HREF="style-sheet.css"&gt;

&lt;body bgcolor="#ffffff" text="#000000" marginwidth="0" marginheight="0" topmargin="0" leftmargin="0"&gt;
&lt;table border=0 cellspacing=0 cellpadding=0 width="100%" cellpaddding=0 height="55%"&gt;
&lt;tr valign="top"&gt;

&lt;/td&gt;
&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;TRIM-POT CROSS REFERENCE&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;RECTANGULAR MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BOURNS&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BI&amp;nbsp;TECH&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;DALE-VISHAY&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PHILIPS/MEPCO&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MURATA&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PANASONIC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;SPECTROL&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MILSPEC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;&lt;TD&gt;&amp;nbsp;&lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3 &gt;
      3005P&lt;BR&gt;
      3006P&lt;BR&gt;
      3006W&lt;BR&gt;
      3006Y&lt;BR&gt;
      3009P&lt;BR&gt;
      3009W&lt;BR&gt;
      3009Y&lt;BR&gt;
      3057J&lt;BR&gt;
      3057L&lt;BR&gt;
      3057P&lt;BR&gt;
      3057Y&lt;BR&gt;
      3059J&lt;BR&gt;
      3059L&lt;BR&gt;
      3059P&lt;BR&gt;
      3059Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      89P&lt;BR&gt;
      89W&lt;BR&gt;
      89X&lt;BR&gt;
      89PH&lt;BR&gt;
      76P&lt;BR&gt;
      89XH&lt;BR&gt;
      78SLT&lt;BR&gt;
      78L&amp;nbsp;ALT&lt;BR&gt;
      56P&amp;nbsp;ALT&lt;BR&gt;
      78P&amp;nbsp;ALT&lt;BR&gt;
      T8S&lt;BR&gt;
      78L&lt;BR&gt;
      56P&lt;BR&gt;
      78P&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      T18/784&lt;BR&gt;
      783&lt;BR&gt;
      781&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2199&lt;BR&gt;
      1697/1897&lt;BR&gt;
      1680/1880&lt;BR&gt;
      2187&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      8035EKP/CT20/RJ-20P&lt;BR&gt;
      -&lt;BR&gt;
      RJ-20X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      1211L&lt;BR&gt;
      8012EKQ&amp;nbsp;ALT&lt;BR&gt;
      8012EKR&amp;nbsp;ALT&lt;BR&gt;
      1211P&lt;BR&gt;
      8012EKJ&lt;BR&gt;
      8012EKL&lt;BR&gt;
      8012EKQ&lt;BR&gt;
      8012EKR&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      2101P&lt;BR&gt;
      2101W&lt;BR&gt;
      2101Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2102L&lt;BR&gt;
      2102S&lt;BR&gt;
      2102Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVMCOG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      43P&lt;BR&gt;
      43W&lt;BR&gt;
      43Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      40L&lt;BR&gt;
      40P&lt;BR&gt;
      40Y&lt;BR&gt;
      70Y-T602&lt;BR&gt;
      70L&lt;BR&gt;
      70P&lt;BR&gt;
      70Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SQUARE MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
   &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3250L&lt;BR&gt;
      3250P&lt;BR&gt;
      3250W&lt;BR&gt;
      3250X&lt;BR&gt;
      3252P&lt;BR&gt;
      3252W&lt;BR&gt;
      3252X&lt;BR&gt;
      3260P&lt;BR&gt;
      3260W&lt;BR&gt;
      3260X&lt;BR&gt;
      3262P&lt;BR&gt;
      3262W&lt;BR&gt;
      3262X&lt;BR&gt;
      3266P&lt;BR&gt;
      3266W&lt;BR&gt;
      3266X&lt;BR&gt;
      3290H&lt;BR&gt;
      3290P&lt;BR&gt;
      3290W&lt;BR&gt;
      3292P&lt;BR&gt;
      3292W&lt;BR&gt;
      3292X&lt;BR&gt;
      3296P&lt;BR&gt;
      3296W&lt;BR&gt;
      3296X&lt;BR&gt;
      3296Y&lt;BR&gt;
      3296Z&lt;BR&gt;
      3299P&lt;BR&gt;
      3299W&lt;BR&gt;
      3299X&lt;BR&gt;
      3299Y&lt;BR&gt;
      3299Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64P&amp;nbsp;ALT&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      64X&amp;nbsp;ALT&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66P&lt;BR&gt;
      66W&lt;BR&gt;
      66X&lt;BR&gt;
      67P&lt;BR&gt;
      67W&lt;BR&gt;
      67X&lt;BR&gt;
      67Y&lt;BR&gt;
      67Z&lt;BR&gt;
      68P&lt;BR&gt;
      68W&lt;BR&gt;
      68X&lt;BR&gt;
      67Y&amp;nbsp;ALT&lt;BR&gt;
      67Z&amp;nbsp;ALT&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      5050&lt;BR&gt;
      5091&lt;BR&gt;
      5080&lt;BR&gt;
      5087&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T63YB&lt;BR&gt;
      T63XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      5887&lt;BR&gt;
      5891&lt;BR&gt;
      5880&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T93Z&lt;BR&gt;
      T93YA&lt;BR&gt;
      T93XA&lt;BR&gt;
      T93YB&lt;BR&gt;
      T93XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKW&lt;BR&gt;
      8026EKM&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKB&lt;BR&gt;
      8026EKM&lt;BR&gt;
      1309X&lt;BR&gt;
      1309P&lt;BR&gt;
      1309W&lt;BR&gt;
      8024EKP&lt;BR&gt;
      8024EKW&lt;BR&gt;
      8024EKN&lt;BR&gt;
      RJ-9P/CT9P&lt;BR&gt;
      RJ-9W&lt;BR&gt;
      RJ-9X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3105P/3106P&lt;BR&gt;
      3105W/3106W&lt;BR&gt;
      3105X/3106X&lt;BR&gt;
      3105Y/3106Y&lt;BR&gt;
      3105Z/3105Z&lt;BR&gt;
      3102P&lt;BR&gt;
      3102W&lt;BR&gt;
      3102X&lt;BR&gt;
      3102Y&lt;BR&gt;
      3102Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMCBG&lt;BR&gt;
      EVMCCG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      55-1-X&lt;BR&gt;
      55-4-X&lt;BR&gt;
      55-3-X&lt;BR&gt;
      55-2-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      50-2-X&lt;BR&gt;
      50-4-X&lt;BR&gt;
      50-3-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      64Y&lt;BR&gt;
      64Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3323P&lt;BR&gt;
      3323S&lt;BR&gt;
      3323W&lt;BR&gt;
      3329H&lt;BR&gt;
      3329P&lt;BR&gt;
      3329W&lt;BR&gt;
      3339H&lt;BR&gt;
      3339P&lt;BR&gt;
      3339W&lt;BR&gt;
      3352E&lt;BR&gt;
      3352H&lt;BR&gt;
      3352K&lt;BR&gt;
      3352P&lt;BR&gt;
      3352T&lt;BR&gt;
      3352V&lt;BR&gt;
      3352W&lt;BR&gt;
      3362H&lt;BR&gt;
      3362M&lt;BR&gt;
      3362P&lt;BR&gt;
      3362R&lt;BR&gt;
      3362S&lt;BR&gt;
      3362U&lt;BR&gt;
      3362W&lt;BR&gt;
      3362X&lt;BR&gt;
      3386B&lt;BR&gt;
      3386C&lt;BR&gt;
      3386F&lt;BR&gt;
      3386H&lt;BR&gt;
      3386K&lt;BR&gt;
      3386M&lt;BR&gt;
      3386P&lt;BR&gt;
      3386S&lt;BR&gt;
      3386W&lt;BR&gt;
      3386X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      25P&lt;BR&gt;
      25S&lt;BR&gt;
      25RX&lt;BR&gt;
      82P&lt;BR&gt;
      82M&lt;BR&gt;
      82PA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      91E&lt;BR&gt;
      91X&lt;BR&gt;
      91T&lt;BR&gt;
      91B&lt;BR&gt;
      91A&lt;BR&gt;
      91V&lt;BR&gt;
      91W&lt;BR&gt;
      25W&lt;BR&gt;
      25V&lt;BR&gt;
      25P&lt;BR&gt;
      -&lt;BR&gt;
      25S&lt;BR&gt;
      25U&lt;BR&gt;
      25RX&lt;BR&gt;
      25X&lt;BR&gt;
      72XW&lt;BR&gt;
      72XL&lt;BR&gt;
      72PM&lt;BR&gt;
      72RX&lt;BR&gt;
      -&lt;BR&gt;
      72PX&lt;BR&gt;
      72P&lt;BR&gt;
      72RXW&lt;BR&gt;
      72RXL&lt;BR&gt;
      72X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T7YB&lt;BR&gt;
      T7YA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      TXD&lt;BR&gt;
      TYA&lt;BR&gt;
      TYP&lt;BR&gt;
      -&lt;BR&gt;
      TYD&lt;BR&gt;
      TX&lt;BR&gt;
      -&lt;BR&gt;
      150SX&lt;BR&gt;
      100SX&lt;BR&gt;
      102T&lt;BR&gt;
      101S&lt;BR&gt;
      190T&lt;BR&gt;
      150TX&lt;BR&gt;
      101&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      101SX&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ET6P&lt;BR&gt;
      ET6S&lt;BR&gt;
      ET6X&lt;BR&gt;
      RJ-6W/8014EMW&lt;BR&gt;
      RJ-6P/8014EMP&lt;BR&gt;
      RJ-6X/8014EMX&lt;BR&gt;
      TM7W&lt;BR&gt;
      TM7P&lt;BR&gt;
      TM7X&lt;BR&gt;
      -&lt;BR&gt;
      8017SMS&lt;BR&gt;
      -&lt;BR&gt;
      8017SMB&lt;BR&gt;
      8017SMA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      CT-6W&lt;BR&gt;
      CT-6H&lt;BR&gt;
      CT-6P&lt;BR&gt;
      CT-6R&lt;BR&gt;
      -&lt;BR&gt;
      CT-6V&lt;BR&gt;
      CT-6X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKV&lt;BR&gt;
      -&lt;BR&gt;
      8038EKX&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKP&lt;BR&gt;
      8038EKZ&lt;BR&gt;
      8038EKW&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3321H&lt;BR&gt;
      3321P&lt;BR&gt;
      3321N&lt;BR&gt;
      1102H&lt;BR&gt;
      1102P&lt;BR&gt;
      1102T&lt;BR&gt;
      RVA0911V304A&lt;BR&gt;
      -&lt;BR&gt;
      RVA0911H413A&lt;BR&gt;
      RVG0707V100A&lt;BR&gt;
      RVA0607V(H)306A&lt;BR&gt;
      RVA1214H213A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3104B&lt;BR&gt;
      3104C&lt;BR&gt;
      3104F&lt;BR&gt;
      3104H&lt;BR&gt;
      -&lt;BR&gt;
      3104M&lt;BR&gt;
      3104P&lt;BR&gt;
      3104S&lt;BR&gt;
      3104W&lt;BR&gt;
      3104X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      EVMQ0G&lt;BR&gt;
      EVMQIG&lt;BR&gt;
      EVMQ3G&lt;BR&gt;
      EVMS0G&lt;BR&gt;
      EVMQ0G&lt;BR&gt;
      EVMG0G&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMK4GA00B&lt;BR&gt;
      EVM30GA00B&lt;BR&gt;
      EVMK0GA00B&lt;BR&gt;
      EVM38GA00B&lt;BR&gt;
      EVMB6&lt;BR&gt;
      EVLQ0&lt;BR&gt;
      -&lt;BR&gt;
      EVMMSG&lt;BR&gt;
      EVMMBG&lt;BR&gt;
      EVMMAG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMMCS&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM0&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM3&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      62-3-1&lt;BR&gt;
      62-1-2&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67R&lt;BR&gt;
      -&lt;BR&gt;
      67P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67X&lt;BR&gt;
      63V&lt;BR&gt;
      63S&lt;BR&gt;
      63M&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63H&lt;BR&gt;
      63P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;&amp;nbsp;&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=3&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT color="#0000FF" SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SMD TRIM-POT CROSS REFERENCE&lt;/B&gt;&lt;/FONT&gt;
      &lt;P&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3224G&lt;BR&gt;
      3224J&lt;BR&gt;
      3224W&lt;BR&gt;
      3269P&lt;BR&gt;
      3269W&lt;BR&gt;
      3269X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      44G&lt;BR&gt;
      44J&lt;BR&gt;
      44W&lt;BR&gt;
      84P&lt;BR&gt;
      84W&lt;BR&gt;
      84X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST63Z&lt;BR&gt;
      ST63Y&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST5P&lt;BR&gt;
      ST5W&lt;BR&gt;
      ST5X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3314G&lt;BR&gt;
      3314J&lt;BR&gt;
      3364A/B&lt;BR&gt;
      3364C/D&lt;BR&gt;
      3364W/X&lt;BR&gt;
      3313G&lt;BR&gt;
      3313J&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      23B&lt;BR&gt;
      23A&lt;BR&gt;
      21X&lt;BR&gt;
      21W&lt;BR&gt;
      -&lt;BR&gt;
      22B&lt;BR&gt;
      22A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST5YL/ST53YL&lt;BR&gt;
      ST5YJ/5T53YJ&lt;BR&gt;
      ST-23A&lt;BR&gt;
      ST-22B&lt;BR&gt;
      ST-22&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST-4B&lt;BR&gt;
      ST-4A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST-3B&lt;BR&gt;
      ST-3A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVM-6YS&lt;BR&gt;
      EVM-1E&lt;BR&gt;
      EVM-1G&lt;BR&gt;
      EVM-1D&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      G4B&lt;BR&gt;
      G4A&lt;BR&gt;
      TR04-3S1&lt;BR&gt;
      TRG04-2S1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      DVR-43A&lt;BR&gt;
      CVR-42C&lt;BR&gt;
      CVR-42A/C&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;
&lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;ALT =&amp;nbsp;ALTERNATE&lt;/B&gt;&lt;/FONT&gt;
&lt;P&gt;

&amp;nbsp;
&lt;P&gt;
&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;
&lt;/BODY&gt;&lt;/HTML&gt;</description>
<packages>
<package name="M0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.10 W</description>
</package>
<package name="C0805K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0805 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 2012</description>
</package>
</packages>
</library>
<library name="SD socket">
<packages>
<package name="SDSOCKET">
</package>
</packages>
</library>
<library name="SparkFun-AnalogIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of analog ICs- DACs, ADCs, video chips, op-amps, and others.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt;Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TSSOP-14">
</package>
</packages>
</library>
<library name="74xx-eu">
<description>&lt;b&gt;TTL Devices, 74xx Series with European Symbols&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Texas Instruments &lt;i&gt;TTL Data Book&lt;/i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;Volume 1, 1996.
&lt;li&gt;TTL Data Book, Volume 2 , 1993
&lt;li&gt;National Seminconductor Databook 1990, ALS/LS Logic
&lt;li&gt;ttl 74er digital data dictionary, ECA Electronic + Acustic GmbH, ISBN 3-88109-032-0
&lt;li&gt;http://icmaster.com/ViewCompare.asp
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SO14">
<description>&lt;b&gt;Small Outline package&lt;/b&gt; 150 mil</description>
</package>
</packages>
</library>
<library name="maxim">
<description>&lt;b&gt;Maxim Components&lt;/b&gt;&lt;p&gt;

&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SO16L">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; .300 SIOC&lt;p&gt;
Source: http://www.maxim-ic.com/cgi-bin/packages?pkg=16%2FSOIC%2E300&amp;Type=Max</description>
</package>
</packages>
</library>
<library name="LIBstereoaudiojack">
<packages>
<package name="AUDIO-JACK-CUI-353X">
</package>
</packages>
</library>
<library name="con-usb-3">
<packages>
<package name="USB-A-H">
<description>&lt;b&gt;USB Series A Hole Mounted&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-ml">
<description>&lt;b&gt;Harting  Connectors&lt;/b&gt;&lt;p&gt;
Low profile connectors, straight&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="ML14">
<description>&lt;b&gt;HARTING&lt;/b&gt;</description>
</package>
<package name="ML40">
<description>&lt;b&gt;HARTING&lt;/b&gt;</description>
</package>
<package name="ML10">
<description>&lt;b&gt;HARTING&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="CHIP-LED0805">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB R99A&lt;br&gt;
Source: http://www.osram.convergy.de/ ... lb_r99a.pdf</description>
</package>
</packages>
</library>
<library name="transistor-npn">
<description>&lt;b&gt;NPN Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23-BEC">
<description>TO-236 ITT Intermetall</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R17" library="rcl" package="M0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="rcl" package="M0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="rcl" package="M0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="rcl" package="M0805" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="rcl" package="M0805" value="1k-10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R21" library="rcl" package="M0805" value="1k-10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="rcl" package="M0805" value="2K 1%">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="rcl" package="M0805" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="rcl" package="M0805" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="XTL_50MHZ" library="crystal" package="SG-636" value="50MHz">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C48" library="rcl" package="C0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C45" library="rcl" package="C0805" value="0.047uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C46" library="rcl" package="C0805" value="0.047uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="rcl" package="C0805" value="2.2uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C47" library="rcl" package="C0805" value="0.022uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C51" library="rcl" package="C0805" value="0.0047uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C44" library="rcl" package="C0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C43" library="rcl" package="C0805" value="0.022uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C50" library="rcl" package="C0805" value="0.022uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C42" library="rcl" package="C0805" value="0.01uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VGA" library="SparkFun-Connectors" package="DB15" value="DB15">
<attribute name="VALUE"/>
</element>
<element name="VIDEODACSA" library="Analog Devices_By_element14_Batch_1" package="QFP50P900X900X120-49N" value="U5">
<attribute name="VALUE"/>
</element>
<element name="R8" library="rcl" package="M0805" value="75">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="rcl" package="M0805" value="75">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="rcl" package="M0805" value="75">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="rcl" package="C0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="rcl" package="M0805" value="348">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="rcl" package="C0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="rcl" package="C0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="rcl" package="C0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="rcl" package="C0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="rcl" package="C0805" value="0.01uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R25" library="rcl" package="R0805" value="22">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R27" library="rcl" package="R0805" value="22">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R29" library="rcl" package="R0805" value="22">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R31" library="rcl" package="R0805" value="22">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R26" library="rcl" package="R0805" value="15k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R28" library="rcl" package="R0805" value="15k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R30" library="rcl" package="R0805" value="15k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R32" library="rcl" package="R0805" value="15k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R42" library="rcl" package="M0805" value="47K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R41" library="rcl" package="M0805" value="47K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R40" library="rcl" package="M0805" value="47K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C23" library="rcl" package="C0805" value="10nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C26" library="rcl" package="C0805" value="10nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R38" library="rcl" package="M0805" value="560">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R36" library="rcl" package="M0805" value="560">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN37" library="resistor-array" package="743-8" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SDRAM" library="sdram" package="TSOP54" value="U8">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="3.3V" library="Exar_By_element14_Batch_1" package="SOT95P280X145-5N" value="U1">
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="OC_NEWARK" value="84R4417"/>
<attribute name="MPN" value="SPX3819M5-L-5-0"/>
<attribute name="SUPPLIER" value="EXAR"/>
<attribute name="OC_FARNELL" value="1829408"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="2.5V" library="Exar_By_element14_Batch_1" package="SOT95P280X145-5N" value="U2">
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="OC_NEWARK" value="84R4417"/>
<attribute name="MPN" value="SPX3819M5-L-5-0"/>
<attribute name="SUPPLIER" value="EXAR"/>
<attribute name="OC_FARNELL" value="1829408"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="1.1V" library="Exar_By_element14_Batch_1" package="SOT95P280X145-5N" value="U3">
<attribute name="PACKAGE" value="SOT-23-5"/>
<attribute name="OC_NEWARK" value="84R4417"/>
<attribute name="MPN" value="SPX3819M5-L-5-0"/>
<attribute name="SUPPLIER" value="EXAR"/>
<attribute name="OC_FARNELL" value="1829408"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="rcl" package="L3225M" value="1uH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L2" library="rcl" package="L3225M" value="1uH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L3" library="rcl" package="L3225M" value="1uH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="rcl" package="C0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="rcl" package="C0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="rcl" package="C0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="rcl" package="C0805" value="22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="rcl" package="C0805" value="22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="rcl" package="C0805" value="22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C19" library="rcl" package="C0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="cyclonev_f484" package="CYCLONEVF484V2" value="U7"/>
<element name="C49" library="rcl" package="C0805" value="0.01uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="rcl" package="C0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="rcl" package="R0805" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="rcl" package="C0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="rcl" package="C0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="rcl" package="R0805" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="rcl" package="R0805" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="rcl" package="R0805" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PF1" library="rcl" package="R1206" value="1A">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ADC" library="adc" package="SOT95P280X145-5N" value="U4">
<attribute name="VALUE"/>
</element>
<element name="R35" library="rcl" package="M0805" value="560">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R37" library="rcl" package="M0805" value="560">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="rcl" package="C0805" value="10nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C25" library="rcl" package="C0805" value="10nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R39" library="rcl" package="M0805" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C21" library="rcl" package="C1206" value="100uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C24" library="rcl" package="C1206" value="100uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S-VIDEO_COMP" library="con-yamaichi" package="MDIN04SS" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C9" library="rcl" package="C0805" value="15pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="rcl" package="R0805" value="240">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="rcl" package="R0805" value="200">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN22" library="resistor-array" package="743-8" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN23" library="resistor-array" package="743-8" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN28" library="resistor-array" package="743-8" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN29" library="resistor-array" package="743-8" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN35" library="resistor-array" package="743-8" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN36" library="resistor-array" package="743-8" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN24" library="resistor-array" package="743-8" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN25" library="resistor-array" package="743-8" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN26" library="resistor-array" package="743-8" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN27" library="resistor-array" package="743-8" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN30" library="resistor-array" package="743-8" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN31" library="resistor-array" package="743-8" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN32" library="resistor-array" package="743-8" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN33" library="resistor-array" package="743-8" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN34" library="resistor-array" package="743-8" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN13" library="resistor-array" package="743-8" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN14" library="resistor-array" package="743-8" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN15" library="resistor-array" package="743-8" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN16" library="resistor-array" package="743-8" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN17" library="resistor-array" package="743-8" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN18" library="resistor-array" package="743-8" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN19" library="resistor-array" package="743-8" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN20" library="resistor-array" package="743-8" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN21" library="resistor-array" package="743-8" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$5" library="header127" package="HDR_141_36" value="HDR_SMALL_36_DEV_LALIGNED"/>
<element name="C27" library="rcl" package="C0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SPI" library="epcs" package="EPCS_BOTH" value="U6">
<attribute name="PACKAGE" value="SOIC-8"/>
<attribute name="OC_NEWARK" value="12T1359"/>
<attribute name="MPN" value="AT25320B-SSHL-B"/>
<attribute name="SUPPLIER" value="Atmel"/>
<attribute name="OC_FARNELL" value="1841578"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="rcl" package="M0805" value="2k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="rcl" package="M0805" value="2k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="rcl" package="C0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="HDMI" library="raspberrypi_cm" package="HDMI" value="HDMI">
<attribute name="NAME"/>
</element>
<element name="RN1" library="resistor-array" package="743-8" value="270">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN2" library="resistor-array" package="743-8" value="270">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="jumper" package="JP2" value="">
<attribute name="VALUE"/>
</element>
<element name="H1" library="holes" package="3,6-PAD" value="MOUNT-PAD-ROUND3.6"/>
<element name="H2" library="holes" package="3,6-PAD" value="MOUNT-PAD-ROUND3.6"/>
<element name="H3" library="holes" package="3,6-PAD" value="MOUNT-PAD-ROUND3.6"/>
<element name="H4" library="holes" package="3,6-PAD" value="MOUNT-PAD-ROUND3.6"/>
<element name="U$6" library="molex_ps" package="MOLEX_PS" value="MOLEX_PS"/>
<element name="RESET" library="jumper" package="JP1" value="RESET">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PF2" library="rcl" package="R1206" value="500mA">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PF4" library="rcl" package="R1206" value="500mA">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R34" library="resistor" package="M0805" value="2k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TR2" library="transistor-pnp" package="SOT23-BEC" value="MOT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R33" library="resistor" package="M0805" value="2k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="QS3384" library="quickswitch" package="TSSOP24" value="U9">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C20" library="resistor" package="C0805K" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="quickswitch" package="SOD123" value="1N4148">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PF3" library="rcl" package="R1206" value="500mA">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN5" library="resistor-array" package="743-8" value="4K7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN6" library="resistor-array" package="743-8" value="4K7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="quickswitch" package="TSSOP24" value="U14">
<attribute name="VALUE"/>
</element>
<element name="IC2" library="quickswitch" package="TSSOP24" value="U15">
<attribute name="VALUE"/>
</element>
<element name="IC3" library="quickswitch" package="TSSOP24" value="U16">
<attribute name="VALUE"/>
</element>
<element name="IC4" library="quickswitch" package="TSSOP24" value="U17">
<attribute name="VALUE"/>
</element>
<element name="D3" library="quickswitch" package="SOD123" value="1N4148">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C38" library="resistor" package="C0805K" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C39" library="resistor" package="C0805K" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C40" library="resistor" package="C0805K" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C41" library="resistor" package="C0805K" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R51" library="resistor" package="M0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R50" library="resistor" package="M0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R55" library="resistor" package="M0805" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R54" library="resistor" package="M0805" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R52" library="resistor" package="M0805" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R53" library="resistor" package="M0805" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SD" library="SD socket" package="SDSOCKET" value="">
<attribute name="VALUE"/>
</element>
<element name="IC5" library="quickswitch" package="TSSOP24" value="U10">
<attribute name="VALUE"/>
</element>
<element name="D2" library="quickswitch" package="SOD123" value="1N4148">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C28" library="resistor" package="C0805K" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JOY2" library="con-subd" package="M09HP" value="JOYSTICK2">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JOY1" library="con-subd" package="M09HP" value="JOYSTICK1">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R44" library="resistor" package="M0805" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R43" library="resistor" package="M0805" value="4.7k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN3" library="resistor-array" package="743-8" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN4" library="resistor-array" package="743-8" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="H6" library="holes" package="3,6-PAD" value="MOUNT-PAD-ROUND3.6"/>
<element name="H7" library="holes" package="3,6-PAD" value="MOUNT-PAD-ROUND3.6"/>
<element name="LM339" library="SparkFun-AnalogIC" package="TSSOP-14" value="U11">
<attribute name="DESC" value="IC, Quad Comparator"/>
<attribute name="MANUF" value="Texas Instruments"/>
<attribute name="SUPPLIER" value="Digikey:296-6607-1-ND"/>
<attribute name="PARTNUM" value="LM339PWR"/>
<attribute name="VALSTAT" value="PARTNUM"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R45" library="rcl" package="R0805" value="1.2K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R46" library="rcl" package="R0805" value="2.1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="74HCT03" library="74xx-eu" package="SO14" value="U12">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="RN8" library="resistor-array" package="743-8" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN9" library="resistor-array" package="743-8" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN7" library="resistor-array" package="743-8" value="4K7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN10" library="resistor-array" package="743-8" value="4K7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN11" library="resistor-array" package="743-8" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C29" library="resistor" package="C0805K" value="0.047uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C30" library="resistor" package="C0805K" value="0.047uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C32" library="resistor" package="C0805K" value="0.047uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C31" library="resistor" package="C0805K" value="0.047uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RN12" library="resistor-array" package="743-8" value="4K7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MAX232" library="maxim" package="SO16L" value="U13">
<attribute name="OC_NEWARK" value="67K4440"/>
<attribute name="MPN" value="MAX232ECWE+"/>
<attribute name="MF" value="MAXIM"/>
<attribute name="OC_FARNELL" value="9724435"/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C34" library="resistor" package="C0805K" value="1UF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C33" library="resistor" package="C0805K" value="1UF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X2" library="con-subd" package="F09V" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="C35" library="resistor" package="C0805K" value="1UF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C36" library="resistor" package="C0805K" value="1UF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="LIBstereoaudiojack" package="AUDIO-JACK-CUI-353X" value="AUDIO-JACK2CUI"/>
<element name="X1" library="con-usb-3" package="USB-A-H" value=""/>
<element name="X3" library="con-usb-3" package="USB-A-H" value=""/>
<element name="GPIO_B" library="con-ml" package="ML14" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R47" library="resistor" package="M0805" value="330">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R48" library="resistor" package="M0805" value="330">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RX" library="led" package="CHIP-LED0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TX" library="led" package="CHIP-LED0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R22" library="rcl" package="R0805" value="82">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R23" library="rcl" package="R0805" value="56">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R24" library="rcl" package="R0805" value="56">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="3V3" library="led" package="CHIP-LED0805" value="Red">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="2V5" library="led" package="CHIP-LED0805" value="Green">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="1V1" library="led" package="CHIP-LED0805" value="White">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TR1" library="transistor-npn" package="SOT23-BEC" value="BC817-16LT1SMD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="3.3/2.5/1.1/GND" library="pinhead" package="1X04" value="J2">
<attribute name="VALUE"/>
</element>
<element name="MIC_IN_SEL" library="jumper" package="JP3Q" value="J1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="P.B.I._INTERFACE" library="con-ml" package="ML40" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="S.I.O._INTERFACE" library="con-ml" package="ML10" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JTAG" library="con-ml" package="ML10" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="GPIO_A" library="con-ml" package="ML40" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="USB_A_B" library="con-ml" package="ML10" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="AC97_AUDIO" library="con-ml" package="ML10" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RESET_LED" library="jumper" package="JP1" value="RESET">
<attribute name="VALUE"/>
</element>
<element name="R25A" library="rcl" package="M0805" value="560">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C30A" library="resistor" package="C0805K" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C29A" library="resistor" package="C0805K" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="H5" library="holes" package="3,6-PAD" value="MOUNT-PAD-ROUND3.6"/>
<element name="R49" library="resistor" package="M0805" value="330">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="R20" pad="2"/>
<contactref element="R14" pad="2"/>
<contactref element="XTL_50MHZ" pad="P$2"/>
<contactref element="C46" pad="1"/>
<contactref element="C45" pad="1"/>
<contactref element="C48" pad="1"/>
<contactref element="C44" pad="2"/>
<contactref element="C43" pad="2"/>
<contactref element="C50" pad="2"/>
<contactref element="C42" pad="2"/>
<contactref element="C51" pad="1"/>
<contactref element="C47" pad="1"/>
<contactref element="C18" pad="1"/>
<contactref element="VIDEODACSA" pad="33"/>
<contactref element="VIDEODACSA" pad="31"/>
<contactref element="VIDEODACSA" pad="27"/>
<contactref element="VIDEODACSA" pad="1"/>
<contactref element="VIDEODACSA" pad="40"/>
<contactref element="VIDEODACSA" pad="39"/>
<contactref element="VIDEODACSA" pad="26"/>
<contactref element="VIDEODACSA" pad="25"/>
<contactref element="VIDEODACSA" pad="15"/>
<contactref element="VIDEODACSA" pad="14"/>
<contactref element="VIDEODACSA" pad="2"/>
<contactref element="VGA" pad="5"/>
<contactref element="R8" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="C10" pad="2"/>
<contactref element="R5" pad="1"/>
<contactref element="C15" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="R28" pad="2"/>
<contactref element="R26" pad="2"/>
<contactref element="R30" pad="2"/>
<contactref element="R32" pad="2"/>
<contactref element="SDRAM" pad="54"/>
<contactref element="SDRAM" pad="28"/>
<contactref element="SDRAM" pad="41"/>
<contactref element="SDRAM" pad="6"/>
<contactref element="SDRAM" pad="12"/>
<contactref element="SDRAM" pad="46"/>
<contactref element="SDRAM" pad="52"/>
<contactref element="1.1V" pad="2"/>
<contactref element="2.5V" pad="2"/>
<contactref element="3.3V" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C19" pad="2"/>
<contactref element="VGA" pad="8"/>
<contactref element="VGA" pad="10"/>
<contactref element="VGA" pad="6"/>
<contactref element="VGA" pad="7"/>
<contactref element="VIDEODACSA" pad="12"/>
<contactref element="U$1" pad="B2"/>
<contactref element="U$1" pad="H4"/>
<contactref element="U$1" pad="M10"/>
<contactref element="U$1" pad="A21"/>
<contactref element="U$1" pad="T1"/>
<contactref element="U$1" pad="AB9"/>
<contactref element="U$1" pad="AB19"/>
<contactref element="U$1" pad="K1"/>
<contactref element="U$1" pad="F5"/>
<contactref element="U$1" pad="P10"/>
<contactref element="U$1" pad="R3"/>
<contactref element="U$1" pad="E3"/>
<contactref element="U$1" pad="P4"/>
<contactref element="U$1" pad="W4"/>
<contactref element="U$1" pad="N15"/>
<contactref element="U$1" pad="M2"/>
<contactref element="U$1" pad="M14"/>
<contactref element="U$1" pad="C17"/>
<contactref element="U$1" pad="H1"/>
<contactref element="U$1" pad="K2"/>
<contactref element="U$1" pad="L3"/>
<contactref element="U$1" pad="F16"/>
<contactref element="U$1" pad="AA4"/>
<contactref element="U$1" pad="E13"/>
<contactref element="U$1" pad="N13"/>
<contactref element="U$1" pad="N5"/>
<contactref element="U$1" pad="Y1"/>
<contactref element="U$1" pad="N17"/>
<contactref element="U$1" pad="L15"/>
<contactref element="U$1" pad="U5"/>
<contactref element="U$1" pad="L11"/>
<contactref element="U$1" pad="D10"/>
<contactref element="U$1" pad="L21"/>
<contactref element="U$1" pad="C4"/>
<contactref element="U$1" pad="H15"/>
<contactref element="U$1" pad="T2"/>
<contactref element="U$1" pad="Y18"/>
<contactref element="U$1" pad="E4"/>
<contactref element="U$1" pad="F2"/>
<contactref element="U$1" pad="M4"/>
<contactref element="U$1" pad="D1"/>
<contactref element="U$1" pad="M1"/>
<contactref element="U$1" pad="H7"/>
<contactref element="U$1" pad="V1"/>
<contactref element="U$1" pad="K12"/>
<contactref element="U$1" pad="C3"/>
<contactref element="U$1" pad="H12"/>
<contactref element="U$1" pad="K14"/>
<contactref element="U$1" pad="J3"/>
<contactref element="U$1" pad="B14"/>
<contactref element="U$1" pad="Y2"/>
<contactref element="U$1" pad="N11"/>
<contactref element="U$1" pad="F1"/>
<contactref element="U$1" pad="N3"/>
<contactref element="U$1" pad="W3"/>
<contactref element="U$1" pad="P2"/>
<contactref element="U$1" pad="V2"/>
<contactref element="U$1" pad="H3"/>
<contactref element="U$1" pad="H22"/>
<contactref element="U$1" pad="AB14"/>
<contactref element="U$1" pad="G9"/>
<contactref element="U$1" pad="R13"/>
<contactref element="U$1" pad="G4"/>
<contactref element="U$1" pad="V17"/>
<contactref element="U$1" pad="D2"/>
<contactref element="U$1" pad="U9"/>
<contactref element="U$1" pad="U4"/>
<contactref element="U$1" pad="V12"/>
<contactref element="U$1" pad="J20"/>
<contactref element="U$1" pad="AB2"/>
<contactref element="U$1" pad="K8"/>
<contactref element="U$1" pad="H2"/>
<contactref element="U$1" pad="G19"/>
<contactref element="U$1" pad="L5"/>
<contactref element="U$1" pad="B9"/>
<contactref element="U$1" pad="A11"/>
<contactref element="U$1" pad="U3"/>
<contactref element="U$1" pad="F6"/>
<contactref element="U$1" pad="AA6"/>
<contactref element="U$1" pad="J5"/>
<contactref element="U$1" pad="N7"/>
<contactref element="U$1" pad="P1"/>
<contactref element="U$1" pad="D5"/>
<contactref element="U$1" pad="V7"/>
<contactref element="U$1" pad="B1"/>
<contactref element="U$1" pad="K10"/>
<contactref element="U$1" pad="C5"/>
<contactref element="U$1" pad="AB1"/>
<contactref element="U$1" pad="K4"/>
<contactref element="U$1" pad="T16"/>
<contactref element="U$1" pad="F17"/>
<contactref element="U$1" pad="T21"/>
<contactref element="U$1" pad="J15"/>
<contactref element="U$1" pad="G3"/>
<contactref element="U$1" pad="AA11"/>
<contactref element="U$1" pad="Y5"/>
<contactref element="U$1" pad="D20"/>
<contactref element="U$1" pad="AA3"/>
<contactref element="U$1" pad="N22"/>
<contactref element="U$1" pad="V22"/>
<contactref element="U$1" pad="L13"/>
<contactref element="U$1" pad="V4"/>
<contactref element="U$1" pad="M12"/>
<contactref element="U$1" pad="A2"/>
<contactref element="U$1" pad="E5"/>
<contactref element="U$1" pad="G5"/>
<contactref element="C49" pad="2"/>
<contactref element="C17" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="ADC" pad="2"/>
<contactref element="C26" pad="1"/>
<contactref element="C23" pad="2"/>
<contactref element="C22" pad="2"/>
<contactref element="C25" pad="1"/>
<contactref element="S-VIDEO_COMP" pad="1"/>
<contactref element="S-VIDEO_COMP" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="C27" pad="2"/>
<contactref element="SPI" pad="4"/>
<contactref element="SPI" pad="L$10"/>
<contactref element="C16" pad="2"/>
<contactref element="HDMI" pad="2"/>
<contactref element="HDMI" pad="5"/>
<contactref element="HDMI" pad="8"/>
<contactref element="HDMI" pad="11"/>
<contactref element="HDMI" pad="17"/>
<contactref element="HDMI" pad="P$1"/>
<contactref element="HDMI" pad="P$2"/>
<contactref element="HDMI" pad="P$3"/>
<contactref element="HDMI" pad="P$4"/>
<contactref element="H1" pad="B3,6"/>
<contactref element="H2" pad="B3,6"/>
<contactref element="H3" pad="B3,6"/>
<contactref element="H4" pad="B3,6"/>
<contactref element="U$6" pad="-"/>
<contactref element="RESET" pad="1"/>
<contactref element="QS3384" pad="21"/>
<contactref element="QS3384" pad="22"/>
<contactref element="QS3384" pad="23"/>
<contactref element="QS3384" pad="20"/>
<contactref element="QS3384" pad="1"/>
<contactref element="QS3384" pad="13"/>
<contactref element="QS3384" pad="12"/>
<contactref element="C20" pad="2"/>
<contactref element="IC1" pad="12"/>
<contactref element="IC2" pad="12"/>
<contactref element="IC3" pad="12"/>
<contactref element="IC4" pad="12"/>
<contactref element="IC4" pad="13"/>
<contactref element="IC4" pad="17"/>
<contactref element="IC4" pad="21"/>
<contactref element="IC4" pad="22"/>
<contactref element="IC4" pad="18"/>
<contactref element="IC2" pad="13"/>
<contactref element="IC2" pad="1"/>
<contactref element="IC3" pad="1"/>
<contactref element="IC3" pad="13"/>
<contactref element="IC4" pad="1"/>
<contactref element="IC1" pad="1"/>
<contactref element="IC1" pad="13"/>
<contactref element="C41" pad="2"/>
<contactref element="C38" pad="2"/>
<contactref element="C39" pad="2"/>
<contactref element="C40" pad="2"/>
<contactref element="IC4" pad="19"/>
<contactref element="IC4" pad="20"/>
<contactref element="IC4" pad="23"/>
<contactref element="IC4" pad="16"/>
<contactref element="R50" pad="1"/>
<contactref element="R51" pad="1"/>
<contactref element="SD" pad="3"/>
<contactref element="SD" pad="11"/>
<contactref element="SD" pad="10"/>
<contactref element="SD" pad="6"/>
<contactref element="IC5" pad="13"/>
<contactref element="C28" pad="1"/>
<contactref element="IC5" pad="1"/>
<contactref element="IC5" pad="12"/>
<contactref element="H6" pad="B3,6"/>
<contactref element="H7" pad="B3,6"/>
<contactref element="R46" pad="1"/>
<contactref element="LM339" pad="12"/>
<contactref element="74HCT03" pad="7"/>
<contactref element="C31" pad="2"/>
<contactref element="C32" pad="2"/>
<contactref element="C30" pad="2"/>
<contactref element="C29" pad="2"/>
<contactref element="X2" pad="5"/>
<contactref element="X1" pad="GND"/>
<contactref element="J3" pad="P$1"/>
<contactref element="X3" pad="GND"/>
<contactref element="GPIO_B" pad="12"/>
<contactref element="GPIO_B" pad="11"/>
<contactref element="2V5" pad="C"/>
<contactref element="3V3" pad="C"/>
<contactref element="R24" pad="2"/>
<contactref element="JOY1" pad="8"/>
<contactref element="JOY2" pad="8"/>
<contactref element="3.3/2.5/1.1/GND" pad="4"/>
<contactref element="JTAG" pad="2"/>
<contactref element="JTAG" pad="10"/>
<contactref element="GPIO_A" pad="12"/>
<contactref element="GPIO_A" pad="30"/>
<contactref element="USB_A_B" pad="7"/>
<contactref element="USB_A_B" pad="8"/>
<contactref element="AC97_AUDIO" pad="2"/>
<contactref element="RESET_LED" pad="2"/>
<contactref element="C30A" pad="2"/>
<contactref element="C29A" pad="2"/>
<contactref element="H5" pad="B3,6"/>
<contactref element="C36" pad="2"/>
<contactref element="C34" pad="2"/>
<contactref element="MAX232" pad="15"/>
</signal>
<signal name="3V3">
<contactref element="R12" pad="2"/>
<contactref element="R17" pad="2"/>
<contactref element="R18" pad="2"/>
<contactref element="R19" pad="2"/>
<contactref element="R21" pad="2"/>
<contactref element="R15" pad="1"/>
<contactref element="R16" pad="1"/>
<contactref element="XTL_50MHZ" pad="P$1"/>
<contactref element="XTL_50MHZ" pad="P$4"/>
<contactref element="C42" pad="1"/>
<contactref element="C50" pad="1"/>
<contactref element="C44" pad="1"/>
<contactref element="C43" pad="1"/>
<contactref element="VIDEODACSA" pad="30"/>
<contactref element="VIDEODACSA" pad="29"/>
<contactref element="VIDEODACSA" pad="13"/>
<contactref element="C11" pad="1"/>
<contactref element="C15" pad="1"/>
<contactref element="C14" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="R42" pad="2"/>
<contactref element="R41" pad="2"/>
<contactref element="R40" pad="2"/>
<contactref element="SDRAM" pad="1"/>
<contactref element="SDRAM" pad="14"/>
<contactref element="SDRAM" pad="27"/>
<contactref element="SDRAM" pad="3"/>
<contactref element="SDRAM" pad="9"/>
<contactref element="SDRAM" pad="43"/>
<contactref element="SDRAM" pad="49"/>
<contactref element="L1" pad="2"/>
<contactref element="3.3V" pad="4"/>
<contactref element="C6" pad="1"/>
<contactref element="C19" pad="1"/>
<contactref element="VIDEODACSA" pad="38"/>
<contactref element="U$1" pad="L6"/>
<contactref element="U$1" pad="J6"/>
<contactref element="U$1" pad="F3"/>
<contactref element="U$1" pad="E8"/>
<contactref element="U$1" pad="AA21"/>
<contactref element="U$1" pad="F21"/>
<contactref element="U$1" pad="R18"/>
<contactref element="U$1" pad="G7"/>
<contactref element="U$1" pad="P20"/>
<contactref element="U$1" pad="W10"/>
<contactref element="U$1" pad="W15"/>
<contactref element="U$1" pad="T6"/>
<contactref element="U$1" pad="R8"/>
<contactref element="U$1" pad="Y8"/>
<contactref element="U$1" pad="C22"/>
<contactref element="U$1" pad="C7"/>
<contactref element="U$1" pad="M19"/>
<contactref element="U$1" pad="W20"/>
<contactref element="U$1" pad="AA16"/>
<contactref element="U$1" pad="C12"/>
<contactref element="U$1" pad="U14"/>
<contactref element="U$1" pad="F11"/>
<contactref element="U$1" pad="K18"/>
<contactref element="U$1" pad="G14"/>
<contactref element="U$1" pad="R1"/>
<contactref element="U$1" pad="D4"/>
<contactref element="U$1" pad="E18"/>
<contactref element="U$1" pad="Y13"/>
<contactref element="U$1" pad="A16"/>
<contactref element="U$1" pad="J1"/>
<contactref element="U$1" pad="U19"/>
<contactref element="U$1" pad="A6"/>
<contactref element="U$1" pad="D15"/>
<contactref element="U$1" pad="B19"/>
<contactref element="U$1" pad="H17"/>
<contactref element="U$1" pad="T11"/>
<contactref element="U$1" pad="Y4"/>
<contactref element="U$1" pad="N18"/>
<contactref element="U$1" pad="D16"/>
<contactref element="U$1" pad="E1"/>
<contactref element="U$1" pad="W6"/>
<contactref element="U$1" pad="R19"/>
<contactref element="U$1" pad="P21"/>
<contactref element="U$1" pad="V8"/>
<contactref element="U$1" pad="J2"/>
<contactref element="U$1" pad="F8"/>
<contactref element="U$1" pad="W11"/>
<contactref element="U$1" pad="M17"/>
<contactref element="U$1" pad="D8"/>
<contactref element="U$1" pad="E11"/>
<contactref element="U$1" pad="W14"/>
<contactref element="U$1" pad="R2"/>
<contactref element="U$1" pad="W17"/>
<contactref element="U$1" pad="D14"/>
<contactref element="U$1" pad="C10"/>
<contactref element="U$1" pad="W12"/>
<contactref element="U$1" pad="AB16"/>
<contactref element="U$1" pad="B8"/>
<contactref element="U$1" pad="C14"/>
<contactref element="U$1" pad="Y7"/>
<contactref element="U$1" pad="L20"/>
<contactref element="U$1" pad="W1"/>
<contactref element="U$1" pad="R20"/>
<contactref element="U$1" pad="Y12"/>
<contactref element="C49" pad="1"/>
<contactref element="C17" pad="1"/>
<contactref element="C27" pad="1"/>
<contactref element="SPI" pad="L$2"/>
<contactref element="SPI" pad="8"/>
<contactref element="R13" pad="2"/>
<contactref element="R11" pad="1"/>
<contactref element="ADC" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="SD" pad="4"/>
<contactref element="R45" pad="2"/>
<contactref element="GPIO_B" pad="13"/>
<contactref element="RN12" pad="8"/>
<contactref element="RN12" pad="5"/>
<contactref element="RN12" pad="6"/>
<contactref element="RN12" pad="7"/>
<contactref element="R22" pad="2"/>
<contactref element="3.3/2.5/1.1/GND" pad="1"/>
<contactref element="JTAG" pad="4"/>
<contactref element="GPIO_A" pad="29"/>
<contactref element="TX" pad="A"/>
<contactref element="RX" pad="A"/>
<contactref element="MAX232" pad="16"/>
</signal>
<signal name="1V1">
<contactref element="C48" pad="2"/>
<contactref element="C45" pad="2"/>
<contactref element="C46" pad="2"/>
<contactref element="U$1" pad="L14"/>
<contactref element="U$1" pad="P13"/>
<contactref element="U$1" pad="N4"/>
<contactref element="U$1" pad="K13"/>
<contactref element="U$1" pad="J4"/>
<contactref element="U$1" pad="K11"/>
<contactref element="U$1" pad="K15"/>
<contactref element="U$1" pad="M13"/>
<contactref element="U$1" pad="P3"/>
<contactref element="U$1" pad="N10"/>
<contactref element="U$1" pad="P11"/>
<contactref element="U$1" pad="M15"/>
<contactref element="U$1" pad="K3"/>
<contactref element="U$1" pad="P15"/>
<contactref element="U$1" pad="J14"/>
<contactref element="U$1" pad="N14"/>
<contactref element="U$1" pad="J16"/>
<contactref element="U$1" pad="L12"/>
<contactref element="U$1" pad="J10"/>
<contactref element="U$1" pad="K5"/>
<contactref element="U$1" pad="J12"/>
<contactref element="U$1" pad="L10"/>
<contactref element="U$1" pad="N12"/>
<contactref element="U$1" pad="L16"/>
<contactref element="U$1" pad="M11"/>
<contactref element="U$1" pad="L4"/>
<contactref element="C9" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="L3" pad="2"/>
<contactref element="C8" pad="1"/>
<contactref element="TR1" pad="B"/>
<contactref element="3.3/2.5/1.1/GND" pad="3"/>
</signal>
<signal name="2V5">
<contactref element="C18" pad="2"/>
<contactref element="C47" pad="2"/>
<contactref element="C51" pad="2"/>
<contactref element="L2" pad="2"/>
<contactref element="2.5V" pad="4"/>
<contactref element="C7" pad="1"/>
<contactref element="U$1" pad="T3"/>
<contactref element="U$1" pad="U18"/>
<contactref element="U$1" pad="H19"/>
<contactref element="U$1" pad="M3"/>
<contactref element="U$1" pad="F4"/>
<contactref element="U$1" pad="T5"/>
<contactref element="U$1" pad="W18"/>
<contactref element="U$1" pad="D18"/>
<contactref element="U$1" pad="D11"/>
<contactref element="U$1" pad="W13"/>
<contactref element="U$1" pad="E6"/>
<contactref element="U$1" pad="W7"/>
<contactref element="U$1" pad="A3"/>
<contactref element="R23" pad="2"/>
<contactref element="3.3/2.5/1.1/GND" pad="2"/>
</signal>
<signal name="CONF_DONE">
<contactref element="R18" pad="1"/>
<contactref element="U$1" pad="K6"/>
</signal>
<signal name="CONFIG_N">
<contactref element="U$1" pad="A4"/>
<contactref element="R12" pad="1"/>
<contactref element="RESET" pad="2"/>
</signal>
<signal name="TCK">
<contactref element="R20" pad="1"/>
<contactref element="U$1" pad="V5"/>
<contactref element="JTAG" pad="1"/>
</signal>
<signal name="TDO">
<contactref element="U$1" pad="M5"/>
<contactref element="JTAG" pad="3"/>
</signal>
<signal name="TMS">
<contactref element="R19" pad="1"/>
<contactref element="U$1" pad="P5"/>
<contactref element="JTAG" pad="5"/>
</signal>
<signal name="TDI">
<contactref element="R21" pad="1"/>
<contactref element="U$1" pad="W5"/>
<contactref element="JTAG" pad="9"/>
</signal>
<signal name="STATUS_N">
<contactref element="R17" pad="1"/>
<contactref element="U$1" pad="H5"/>
</signal>
<signal name="RREF_TL">
<contactref element="R14" pad="1"/>
<contactref element="U$1" pad="A1"/>
</signal>
<signal name="N$6">
<contactref element="U$1" pad="V3"/>
<contactref element="SPI" pad="6"/>
<contactref element="SPI" pad="L$16"/>
</signal>
<signal name="N$7">
<contactref element="U$1" pad="R4"/>
<contactref element="SPI" pad="L$7"/>
<contactref element="SPI" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="U$1" pad="AB3"/>
<contactref element="SPI" pad="L$8"/>
<contactref element="SPI" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="U$1" pad="AB4"/>
<contactref element="SPI" pad="L$15"/>
<contactref element="SPI" pad="5"/>
</signal>
<signal name="N$10">
<contactref element="R16" pad="2"/>
<contactref element="SPI" pad="3"/>
<contactref element="SPI" pad="L$9"/>
</signal>
<signal name="N$11">
<contactref element="R15" pad="2"/>
<contactref element="SPI" pad="7"/>
<contactref element="SPI" pad="L$1"/>
</signal>
<signal name="N$12">
<contactref element="XTL_50MHZ" pad="P$3"/>
<contactref element="U$1" pad="H16"/>
</signal>
<signal name="N$13">
<contactref element="VIDEODACSA" pad="34"/>
<contactref element="VGA" pad="1"/>
<contactref element="R6" pad="2"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="N$14">
<contactref element="VIDEODACSA" pad="32"/>
<contactref element="VGA" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="S-VIDEO_COMP" pad="4"/>
</signal>
<signal name="VGA_R0">
<contactref element="VIDEODACSA" pad="41"/>
<contactref element="U$1" pad="A5"/>
<contactref element="RN1" pad="1"/>
</signal>
<signal name="VGA_R1">
<contactref element="VIDEODACSA" pad="42"/>
<contactref element="U$1" pad="B5"/>
<contactref element="RN1" pad="2"/>
</signal>
<signal name="VGA_R2">
<contactref element="VIDEODACSA" pad="43"/>
<contactref element="U$1" pad="B6"/>
</signal>
<signal name="VGA_R3">
<contactref element="VIDEODACSA" pad="44"/>
<contactref element="U$1" pad="D6"/>
<contactref element="RN1" pad="4"/>
</signal>
<signal name="VGA_R4">
<contactref element="VIDEODACSA" pad="45"/>
<contactref element="U$1" pad="C6"/>
<contactref element="RN1" pad="3"/>
</signal>
<signal name="VGA_R5">
<contactref element="VIDEODACSA" pad="46"/>
<contactref element="U$1" pad="A7"/>
</signal>
<signal name="VGA_R6">
<contactref element="VIDEODACSA" pad="47"/>
<contactref element="U$1" pad="B7"/>
</signal>
<signal name="VGA_R7">
<contactref element="VIDEODACSA" pad="48"/>
<contactref element="U$1" pad="E7"/>
</signal>
<signal name="VGA_G0">
<contactref element="VIDEODACSA" pad="3"/>
<contactref element="U$1" pad="D7"/>
</signal>
<signal name="VGA_G1">
<contactref element="VIDEODACSA" pad="4"/>
<contactref element="U$1" pad="F7"/>
</signal>
<signal name="VGA_G2">
<contactref element="VIDEODACSA" pad="5"/>
<contactref element="U$1" pad="A8"/>
</signal>
<signal name="VGA_G3">
<contactref element="VIDEODACSA" pad="6"/>
<contactref element="U$1" pad="G8"/>
</signal>
<signal name="VGA_G4">
<contactref element="VIDEODACSA" pad="7"/>
<contactref element="U$1" pad="C8"/>
</signal>
<signal name="VGA_G5">
<contactref element="VIDEODACSA" pad="8"/>
<contactref element="U$1" pad="H8"/>
</signal>
<signal name="VGA_G6">
<contactref element="VIDEODACSA" pad="9"/>
<contactref element="U$1" pad="A9"/>
</signal>
<signal name="VGA_G7">
<contactref element="VIDEODACSA" pad="10"/>
<contactref element="U$1" pad="D9"/>
</signal>
<signal name="VGA_B0">
<contactref element="VIDEODACSA" pad="16"/>
<contactref element="U$1" pad="E9"/>
</signal>
<signal name="VGA_B1">
<contactref element="VIDEODACSA" pad="17"/>
<contactref element="U$1" pad="F9"/>
<contactref element="RN2" pad="2"/>
</signal>
<signal name="VGA_B2">
<contactref element="VIDEODACSA" pad="18"/>
<contactref element="U$1" pad="A10"/>
</signal>
<signal name="VGA_B3">
<contactref element="VIDEODACSA" pad="19"/>
<contactref element="U$1" pad="B10"/>
</signal>
<signal name="VGA_B4">
<contactref element="VIDEODACSA" pad="20"/>
<contactref element="U$1" pad="E10"/>
<contactref element="RN2" pad="1"/>
</signal>
<signal name="VGA_B5">
<contactref element="VIDEODACSA" pad="21"/>
<contactref element="U$1" pad="F10"/>
<contactref element="RN2" pad="4"/>
</signal>
<signal name="VGA_B6">
<contactref element="VIDEODACSA" pad="22"/>
<contactref element="U$1" pad="G10"/>
<contactref element="RN2" pad="3"/>
</signal>
<signal name="VGA_B7">
<contactref element="VIDEODACSA" pad="23"/>
<contactref element="U$1" pad="B11"/>
</signal>
<signal name="VGA_BLANK_N">
<contactref element="VIDEODACSA" pad="11"/>
<contactref element="U$1" pad="C9"/>
</signal>
<signal name="VGA_CLK">
<contactref element="VIDEODACSA" pad="24"/>
<contactref element="U$1" pad="G11"/>
</signal>
<signal name="N$16">
<contactref element="VIDEODACSA" pad="36"/>
<contactref element="C10" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="VIDEODACSA" pad="37"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="VIDEODACSA" pad="35"/>
<contactref element="C11" pad="2"/>
</signal>
<signal name="5V0">
<contactref element="2.5V" pad="1"/>
<contactref element="1.1V" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="3.3V" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="HDMI" pad="18"/>
<contactref element="PF1" pad="2"/>
<contactref element="PF2" pad="1"/>
<contactref element="PF4" pad="1"/>
<contactref element="D1" pad="2"/>
<contactref element="TR2" pad="E"/>
<contactref element="R33" pad="1"/>
<contactref element="RN5" pad="1"/>
<contactref element="RN6" pad="4"/>
<contactref element="RN6" pad="3"/>
<contactref element="RN6" pad="2"/>
<contactref element="RN6" pad="1"/>
<contactref element="RN5" pad="4"/>
<contactref element="RN5" pad="3"/>
<contactref element="RN5" pad="2"/>
<contactref element="D3" pad="2"/>
<contactref element="R53" pad="1"/>
<contactref element="R52" pad="1"/>
<contactref element="R55" pad="1"/>
<contactref element="R54" pad="1"/>
<contactref element="R43" pad="2"/>
<contactref element="R44" pad="2"/>
<contactref element="LM339" pad="3"/>
<contactref element="74HCT03" pad="14"/>
<contactref element="GPIO_B" pad="14"/>
<contactref element="D2" pad="2"/>
<contactref element="RN7" pad="1"/>
<contactref element="RN7" pad="2"/>
<contactref element="RN7" pad="3"/>
<contactref element="RN7" pad="4"/>
<contactref element="RN10" pad="8"/>
<contactref element="RN10" pad="7"/>
<contactref element="RN10" pad="6"/>
<contactref element="RN10" pad="5"/>
<contactref element="GPIO_A" pad="11"/>
<contactref element="R25A" pad="1"/>
<contactref element="C30A" pad="1"/>
<contactref element="C29A" pad="1"/>
<contactref element="1V1" pad="A"/>
</signal>
<signal name="N$20">
<contactref element="R26" pad="1"/>
<contactref element="R25" pad="2"/>
<contactref element="X1" pad="D+"/>
<contactref element="USB_A_B" pad="5"/>
</signal>
<signal name="N$23">
<contactref element="R27" pad="2"/>
<contactref element="R28" pad="1"/>
<contactref element="X1" pad="D-"/>
<contactref element="USB_A_B" pad="3"/>
</signal>
<signal name="USB1DP">
<contactref element="R25" pad="1"/>
<contactref element="U$1" pad="V10"/>
</signal>
<signal name="USB1DM">
<contactref element="R27" pad="1"/>
<contactref element="U$1" pad="AA10"/>
</signal>
<signal name="USB2DP">
<contactref element="R29" pad="1"/>
<contactref element="U$1" pad="AB10"/>
</signal>
<signal name="USB2DM">
<contactref element="R31" pad="1"/>
<contactref element="U$1" pad="R11"/>
</signal>
<signal name="AUDIO_RIGHT">
<contactref element="R36" pad="2"/>
<contactref element="U$1" pad="T13"/>
</signal>
<signal name="AUDIO_LEFT">
<contactref element="R38" pad="2"/>
<contactref element="U$1" pad="U13"/>
</signal>
<signal name="SD_DAT2">
<contactref element="U$1" pad="B12"/>
<contactref element="SD" pad="9"/>
</signal>
<signal name="SD_CS">
<contactref element="U$1" pad="D12"/>
<contactref element="SD" pad="1"/>
<contactref element="R40" pad="1"/>
</signal>
<signal name="SD_DETECT">
<contactref element="U$1" pad="E12"/>
<contactref element="SD" pad="3A"/>
</signal>
<signal name="SD_MOSI">
<contactref element="U$1" pad="F12"/>
<contactref element="SD" pad="2"/>
<contactref element="R41" pad="1"/>
</signal>
<signal name="SD_DAT1">
<contactref element="U$1" pad="A13"/>
<contactref element="SD" pad="8"/>
</signal>
<signal name="SD_SCK">
<contactref element="U$1" pad="B13"/>
<contactref element="SD" pad="5"/>
</signal>
<signal name="SD_WRITEPROTECT">
<contactref element="U$1" pad="D13"/>
<contactref element="SD" pad="8A"/>
</signal>
<signal name="SD_MISO">
<contactref element="U$1" pad="C13"/>
<contactref element="SD" pad="7"/>
<contactref element="R42" pad="1"/>
</signal>
<signal name="N$22">
<contactref element="RN13" pad="8"/>
<contactref element="GPIO_A" pad="1"/>
</signal>
<signal name="GPIOA0">
<contactref element="U$1" pad="F15"/>
<contactref element="RN13" pad="1"/>
<contactref element="U$5" pad="P$1"/>
</signal>
<signal name="N$24">
<contactref element="RN13" pad="7"/>
<contactref element="GPIO_A" pad="2"/>
</signal>
<signal name="N$29">
<contactref element="RN13" pad="6"/>
<contactref element="GPIO_A" pad="3"/>
</signal>
<signal name="N$30">
<contactref element="RN13" pad="5"/>
<contactref element="GPIO_A" pad="4"/>
</signal>
<signal name="N$31">
<contactref element="RN14" pad="8"/>
<contactref element="GPIO_A" pad="5"/>
</signal>
<signal name="N$32">
<contactref element="RN14" pad="7"/>
<contactref element="GPIO_A" pad="6"/>
</signal>
<signal name="N$33">
<contactref element="RN14" pad="6"/>
<contactref element="GPIO_A" pad="7"/>
</signal>
<signal name="N$34">
<contactref element="RN14" pad="5"/>
<contactref element="GPIO_A" pad="8"/>
</signal>
<signal name="N$35">
<contactref element="RN15" pad="8"/>
<contactref element="GPIO_A" pad="9"/>
</signal>
<signal name="N$36">
<contactref element="RN15" pad="7"/>
<contactref element="GPIO_A" pad="10"/>
</signal>
<signal name="N$37">
<contactref element="RN15" pad="6"/>
<contactref element="GPIO_A" pad="13"/>
</signal>
<signal name="N$38">
<contactref element="RN15" pad="5"/>
<contactref element="GPIO_A" pad="14"/>
</signal>
<signal name="N$41">
<contactref element="RN16" pad="7"/>
<contactref element="GPIO_A" pad="16"/>
</signal>
<signal name="N$40">
<contactref element="RN16" pad="6"/>
<contactref element="GPIO_A" pad="17"/>
</signal>
<signal name="N$42">
<contactref element="RN16" pad="5"/>
<contactref element="GPIO_A" pad="18"/>
</signal>
<signal name="N$43">
<contactref element="RN17" pad="8"/>
<contactref element="GPIO_A" pad="19"/>
</signal>
<signal name="N$44">
<contactref element="RN17" pad="7"/>
<contactref element="GPIO_A" pad="20"/>
</signal>
<signal name="N$45">
<contactref element="RN17" pad="6"/>
<contactref element="GPIO_A" pad="21"/>
</signal>
<signal name="N$46">
<contactref element="RN17" pad="5"/>
<contactref element="GPIO_A" pad="22"/>
</signal>
<signal name="N$47">
<contactref element="RN18" pad="8"/>
<contactref element="GPIO_A" pad="23"/>
</signal>
<signal name="N$48">
<contactref element="RN18" pad="6"/>
<contactref element="GPIO_A" pad="25"/>
</signal>
<signal name="N$49">
<contactref element="RN18" pad="7"/>
<contactref element="GPIO_A" pad="24"/>
</signal>
<signal name="N$50">
<contactref element="RN18" pad="5"/>
<contactref element="GPIO_A" pad="26"/>
</signal>
<signal name="N$51">
<contactref element="RN19" pad="8"/>
<contactref element="GPIO_A" pad="27"/>
</signal>
<signal name="N$52">
<contactref element="RN19" pad="7"/>
<contactref element="GPIO_A" pad="28"/>
</signal>
<signal name="N$53">
<contactref element="RN19" pad="6"/>
<contactref element="GPIO_A" pad="31"/>
</signal>
<signal name="N$54">
<contactref element="RN19" pad="5"/>
<contactref element="GPIO_A" pad="32"/>
</signal>
<signal name="N$55">
<contactref element="RN20" pad="8"/>
<contactref element="GPIO_A" pad="33"/>
</signal>
<signal name="N$56">
<contactref element="RN20" pad="7"/>
<contactref element="GPIO_A" pad="34"/>
</signal>
<signal name="N$57">
<contactref element="RN20" pad="6"/>
<contactref element="GPIO_A" pad="35"/>
</signal>
<signal name="N$58">
<contactref element="RN20" pad="5"/>
<contactref element="GPIO_A" pad="36"/>
</signal>
<signal name="N$59">
<contactref element="RN21" pad="8"/>
<contactref element="GPIO_A" pad="37"/>
</signal>
<signal name="N$60">
<contactref element="RN21" pad="7"/>
<contactref element="GPIO_A" pad="38"/>
</signal>
<signal name="N$61">
<contactref element="RN21" pad="6"/>
<contactref element="GPIO_A" pad="39"/>
</signal>
<signal name="N$62">
<contactref element="RN21" pad="5"/>
<contactref element="GPIO_A" pad="40"/>
</signal>
<signal name="GPIOA1">
<contactref element="U$1" pad="B16"/>
<contactref element="RN13" pad="2"/>
<contactref element="U$5" pad="P$2"/>
</signal>
<signal name="GPIOA2">
<contactref element="U$1" pad="C16"/>
<contactref element="RN13" pad="3"/>
<contactref element="U$5" pad="P$3"/>
</signal>
<signal name="GPIOA3">
<contactref element="U$1" pad="G17"/>
<contactref element="RN13" pad="4"/>
<contactref element="U$5" pad="P$4"/>
</signal>
<signal name="GPIOA4">
<contactref element="U$1" pad="G16"/>
<contactref element="RN14" pad="1"/>
<contactref element="U$5" pad="P$5"/>
</signal>
<signal name="GPIOA5">
<contactref element="U$1" pad="J18"/>
<contactref element="RN14" pad="2"/>
<contactref element="U$5" pad="P$6"/>
</signal>
<signal name="GPIOA6">
<contactref element="U$1" pad="J17"/>
<contactref element="RN14" pad="3"/>
<contactref element="U$5" pad="P$7"/>
</signal>
<signal name="GPIOA7">
<contactref element="U$1" pad="K21"/>
<contactref element="RN14" pad="4"/>
<contactref element="U$5" pad="P$8"/>
</signal>
<signal name="GPIOA8">
<contactref element="U$1" pad="K20"/>
<contactref element="RN15" pad="1"/>
<contactref element="U$5" pad="P$9"/>
</signal>
<signal name="GPIOA9">
<contactref element="U$1" pad="K16"/>
<contactref element="RN15" pad="2"/>
<contactref element="U$5" pad="P$10"/>
</signal>
<signal name="GPIOA10">
<contactref element="U$1" pad="L19"/>
<contactref element="RN15" pad="3"/>
<contactref element="U$5" pad="P$11"/>
</signal>
<signal name="GPIOA11">
<contactref element="U$1" pad="L17"/>
<contactref element="RN15" pad="4"/>
<contactref element="U$5" pad="P$12"/>
</signal>
<signal name="GPIOA12">
<contactref element="U$1" pad="M21"/>
<contactref element="RN16" pad="1"/>
<contactref element="U$5" pad="P$13"/>
</signal>
<signal name="GPIOA13">
<contactref element="U$1" pad="M20"/>
<contactref element="RN16" pad="2"/>
<contactref element="U$5" pad="P$14"/>
</signal>
<signal name="GPIOA14">
<contactref element="U$1" pad="N21"/>
<contactref element="RN16" pad="3"/>
<contactref element="U$5" pad="P$15"/>
</signal>
<signal name="GPIOA15">
<contactref element="U$1" pad="N20"/>
<contactref element="RN16" pad="4"/>
<contactref element="U$5" pad="P$16"/>
</signal>
<signal name="GPIOA16">
<contactref element="U$1" pad="P22"/>
<contactref element="RN17" pad="1"/>
<contactref element="U$5" pad="P$17"/>
</signal>
<signal name="GPIOA17">
<contactref element="U$1" pad="P19"/>
<contactref element="RN17" pad="2"/>
<contactref element="U$5" pad="P$18"/>
</signal>
<signal name="GPIOA18">
<contactref element="U$1" pad="P16"/>
<contactref element="RN17" pad="3"/>
<contactref element="U$5" pad="P$19"/>
</signal>
<signal name="GPIOA19">
<contactref element="U$1" pad="R21"/>
<contactref element="RN17" pad="4"/>
<contactref element="U$5" pad="P$20"/>
</signal>
<signal name="GPIOA20">
<contactref element="U$1" pad="R16"/>
<contactref element="RN18" pad="1"/>
<contactref element="U$5" pad="P$21"/>
</signal>
<signal name="GPIOA21">
<contactref element="U$1" pad="T19"/>
<contactref element="RN18" pad="2"/>
<contactref element="U$5" pad="P$22"/>
</signal>
<signal name="GPIOA22">
<contactref element="U$1" pad="T18"/>
<contactref element="RN18" pad="3"/>
<contactref element="U$5" pad="P$23"/>
</signal>
<signal name="GPIOA23">
<contactref element="U$1" pad="U22"/>
<contactref element="RN18" pad="4"/>
<contactref element="U$5" pad="P$24"/>
</signal>
<signal name="GPIOA24">
<contactref element="U$1" pad="U20"/>
<contactref element="RN19" pad="1"/>
<contactref element="U$5" pad="P$25"/>
</signal>
<signal name="GPIOA25">
<contactref element="U$1" pad="V19"/>
<contactref element="RN19" pad="2"/>
<contactref element="U$5" pad="P$26"/>
</signal>
<signal name="GPIOA26">
<contactref element="U$1" pad="W22"/>
<contactref element="RN19" pad="3"/>
<contactref element="U$5" pad="P$27"/>
</signal>
<signal name="GPIOA27">
<contactref element="U$1" pad="Y22"/>
<contactref element="RN19" pad="4"/>
<contactref element="U$5" pad="P$28"/>
</signal>
<signal name="GPIOA28">
<contactref element="U$1" pad="AA22"/>
<contactref element="RN20" pad="1"/>
<contactref element="U$5" pad="P$29"/>
</signal>
<signal name="GPIOA29">
<contactref element="U$1" pad="AB21"/>
<contactref element="RN20" pad="2"/>
<contactref element="U$5" pad="P$30"/>
</signal>
<signal name="GPIOA30">
<contactref element="U$1" pad="AA20"/>
<contactref element="RN20" pad="3"/>
<contactref element="U$5" pad="P$31"/>
</signal>
<signal name="GPIOA31">
<contactref element="U$1" pad="AA19"/>
<contactref element="RN20" pad="4"/>
<contactref element="U$5" pad="P$32"/>
</signal>
<signal name="GPIOA32">
<contactref element="U$1" pad="Y19"/>
<contactref element="RN21" pad="1"/>
<contactref element="U$5" pad="P$33"/>
</signal>
<signal name="GPIOA33">
<contactref element="U$1" pad="AA18"/>
<contactref element="RN21" pad="2"/>
<contactref element="U$5" pad="P$34"/>
</signal>
<signal name="GPIOA34">
<contactref element="U$1" pad="AB17"/>
<contactref element="RN21" pad="3"/>
<contactref element="U$5" pad="P$35"/>
</signal>
<signal name="GPIOA35">
<contactref element="U$1" pad="U17"/>
<contactref element="RN21" pad="4"/>
<contactref element="U$5" pad="P$36"/>
</signal>
<signal name="A0">
<contactref element="SDRAM" pad="23"/>
<contactref element="U$1" pad="R6"/>
</signal>
<signal name="A1">
<contactref element="SDRAM" pad="24"/>
<contactref element="U$1" pad="R5"/>
</signal>
<signal name="A2">
<contactref element="SDRAM" pad="25"/>
<contactref element="U$1" pad="T7"/>
</signal>
<signal name="A3">
<contactref element="SDRAM" pad="26"/>
<contactref element="U$1" pad="U6"/>
</signal>
<signal name="A4">
<contactref element="SDRAM" pad="29"/>
<contactref element="U$1" pad="Y10"/>
</signal>
<signal name="A5">
<contactref element="SDRAM" pad="30"/>
<contactref element="U$1" pad="U10"/>
</signal>
<signal name="A6">
<contactref element="SDRAM" pad="31"/>
<contactref element="U$1" pad="T10"/>
</signal>
<signal name="A7">
<contactref element="SDRAM" pad="32"/>
<contactref element="U$1" pad="AA9"/>
</signal>
<signal name="A8">
<contactref element="SDRAM" pad="33"/>
<contactref element="U$1" pad="W9"/>
</signal>
<signal name="A9">
<contactref element="SDRAM" pad="34"/>
<contactref element="U$1" pad="Y9"/>
</signal>
<signal name="A10">
<contactref element="SDRAM" pad="22"/>
<contactref element="U$1" pad="R7"/>
</signal>
<signal name="A11">
<contactref element="SDRAM" pad="35"/>
<contactref element="U$1" pad="V9"/>
</signal>
<signal name="A12">
<contactref element="SDRAM" pad="36"/>
<contactref element="U$1" pad="T9"/>
</signal>
<signal name="BA0">
<contactref element="SDRAM" pad="20"/>
<contactref element="U$1" pad="P7"/>
</signal>
<signal name="BA1">
<contactref element="SDRAM" pad="21"/>
<contactref element="U$1" pad="P6"/>
</signal>
<signal name="SDRAM_UDQM">
<contactref element="SDRAM" pad="39"/>
<contactref element="U$1" pad="U8"/>
</signal>
<signal name="SDRAM_LDQM">
<contactref element="SDRAM" pad="15"/>
<contactref element="U$1" pad="M6"/>
</signal>
<signal name="SDRAM_CLK">
<contactref element="SDRAM" pad="38"/>
<contactref element="U$1" pad="AA8"/>
</signal>
<signal name="CKE">
<contactref element="SDRAM" pad="37"/>
<contactref element="U$1" pad="AB8"/>
</signal>
<signal name="CS_N">
<contactref element="SDRAM" pad="19"/>
<contactref element="U$1" pad="P8"/>
</signal>
<signal name="RAS_N">
<contactref element="SDRAM" pad="18"/>
<contactref element="U$1" pad="N6"/>
</signal>
<signal name="CAS_N">
<contactref element="SDRAM" pad="17"/>
<contactref element="U$1" pad="N8"/>
</signal>
<signal name="WE_N">
<contactref element="SDRAM" pad="16"/>
<contactref element="U$1" pad="N9"/>
</signal>
<signal name="DQ0">
<contactref element="SDRAM" pad="2"/>
<contactref element="U$1" pad="K7"/>
</signal>
<signal name="DQ1">
<contactref element="SDRAM" pad="4"/>
<contactref element="U$1" pad="K9"/>
</signal>
<signal name="DQ2">
<contactref element="SDRAM" pad="5"/>
<contactref element="U$1" pad="J7"/>
</signal>
<signal name="DQ3">
<contactref element="SDRAM" pad="7"/>
<contactref element="U$1" pad="J8"/>
</signal>
<signal name="DQ4">
<contactref element="SDRAM" pad="8"/>
<contactref element="U$1" pad="L8"/>
</signal>
<signal name="DQ5">
<contactref element="SDRAM" pad="10"/>
<contactref element="U$1" pad="L7"/>
</signal>
<signal name="DQ6">
<contactref element="SDRAM" pad="11"/>
<contactref element="U$1" pad="M8"/>
</signal>
<signal name="DQ7">
<contactref element="SDRAM" pad="13"/>
<contactref element="U$1" pad="M7"/>
</signal>
<signal name="DQ8">
<contactref element="SDRAM" pad="42"/>
<contactref element="U$1" pad="W8"/>
</signal>
<signal name="DQ9">
<contactref element="SDRAM" pad="44"/>
<contactref element="U$1" pad="T8"/>
</signal>
<signal name="DQ10">
<contactref element="SDRAM" pad="45"/>
<contactref element="U$1" pad="AB7"/>
</signal>
<signal name="DQ11">
<contactref element="SDRAM" pad="47"/>
<contactref element="U$1" pad="AA7"/>
</signal>
<signal name="DQ12">
<contactref element="SDRAM" pad="48"/>
<contactref element="U$1" pad="U7"/>
</signal>
<signal name="DQ13">
<contactref element="SDRAM" pad="50"/>
<contactref element="U$1" pad="AB6"/>
</signal>
<signal name="DQ14">
<contactref element="SDRAM" pad="51"/>
<contactref element="U$1" pad="V6"/>
</signal>
<signal name="DQ15">
<contactref element="SDRAM" pad="53"/>
<contactref element="U$1" pad="AB5"/>
</signal>
<signal name="N$135">
<contactref element="1.1V" pad="5"/>
<contactref element="L3" pad="1"/>
</signal>
<signal name="N$136">
<contactref element="2.5V" pad="5"/>
<contactref element="L2" pad="1"/>
</signal>
<signal name="N$137">
<contactref element="3.3V" pad="5"/>
<contactref element="L1" pad="1"/>
</signal>
<signal name="N$39">
<contactref element="RN16" pad="8"/>
<contactref element="GPIO_A" pad="15"/>
</signal>
<signal name="VSYNC">
<contactref element="U$1" pad="H11"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="HSYNC">
<contactref element="U$1" pad="C11"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="N$4">
</signal>
<signal name="N$140">
</signal>
<signal name="SDA">
<contactref element="U$1" pad="H6"/>
<contactref element="ADC" pad="4"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="SCL">
<contactref element="U$1" pad="G6"/>
<contactref element="ADC" pad="5"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="5V0FAST">
<contactref element="R1" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="1.1V" pad="3"/>
</signal>
<signal name="5V0SLOW">
<contactref element="R2" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="3.3V" pad="3"/>
<contactref element="2.5V" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="VGA" pad="14"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="VGA" pad="13"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="N$27">
<contactref element="R36" pad="1"/>
<contactref element="C23" pad="1"/>
<contactref element="R35" pad="2"/>
<contactref element="R39" pad="2"/>
</signal>
<signal name="N$28">
<contactref element="R38" pad="1"/>
<contactref element="C26" pad="2"/>
<contactref element="R37" pad="2"/>
<contactref element="R39" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="R35" pad="1"/>
<contactref element="C22" pad="1"/>
<contactref element="C21" pad="2"/>
</signal>
<signal name="N$142">
<contactref element="C25" pad="2"/>
<contactref element="R37" pad="1"/>
<contactref element="C24" pad="2"/>
</signal>
<signal name="N$145">
<contactref element="R4" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="1.1V" pad="4"/>
</signal>
<signal name="N$143">
<contactref element="VIDEODACSA" pad="28"/>
<contactref element="VGA" pad="3"/>
<contactref element="R8" pad="2"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="N$134">
<contactref element="RN1" pad="8"/>
<contactref element="HDMI" pad="1"/>
</signal>
<signal name="N$144">
<contactref element="HDMI" pad="3"/>
<contactref element="RN1" pad="7"/>
</signal>
<signal name="N$146">
<contactref element="RN1" pad="6"/>
<contactref element="HDMI" pad="4"/>
</signal>
<signal name="N$147">
<contactref element="HDMI" pad="6"/>
<contactref element="RN1" pad="5"/>
</signal>
<signal name="N$148">
<contactref element="RN2" pad="8"/>
<contactref element="HDMI" pad="7"/>
</signal>
<signal name="N$149">
<contactref element="HDMI" pad="9"/>
<contactref element="RN2" pad="7"/>
</signal>
<signal name="N$150">
<contactref element="RN2" pad="6"/>
<contactref element="HDMI" pad="10"/>
</signal>
<signal name="N$151">
<contactref element="HDMI" pad="12"/>
<contactref element="RN2" pad="5"/>
</signal>
<signal name="N$152">
<contactref element="S-VIDEO_COMP" pad="3"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="N$138">
<contactref element="C24" pad="1"/>
<contactref element="J3" pad="P$2"/>
<contactref element="AC97_AUDIO" pad="9"/>
</signal>
<signal name="N$141">
<contactref element="C21" pad="1"/>
<contactref element="J3" pad="P$3"/>
<contactref element="AC97_AUDIO" pad="5"/>
</signal>
<signal name="MIC_AC97">
<contactref element="MIC_IN_SEL" pad="2"/>
<contactref element="AC97_AUDIO" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="U$6" pad="+"/>
<contactref element="PF1" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="PF2" pad="2"/>
<contactref element="X1" pad="VBUS"/>
<contactref element="X3" pad="VBUS"/>
<contactref element="USB_A_B" pad="1"/>
<contactref element="USB_A_B" pad="2"/>
</signal>
<signal name="MOTOR_RAW">
<contactref element="U$1" pad="Y11"/>
<contactref element="RN3" pad="1"/>
</signal>
<signal name="COMMAND">
<contactref element="U$1" pad="AB11"/>
<contactref element="RN4" pad="2"/>
</signal>
<signal name="SIO_OUT">
<contactref element="U$1" pad="R12"/>
<contactref element="RN4" pad="1"/>
</signal>
<signal name="SIO_IN">
<contactref element="U$1" pad="U12"/>
<contactref element="RN3" pad="3"/>
</signal>
<signal name="PROCEED">
<contactref element="U$1" pad="U11"/>
<contactref element="RN4" pad="3"/>
</signal>
<signal name="SIO_IRQ">
<contactref element="U$1" pad="T12"/>
<contactref element="RN3" pad="4"/>
</signal>
<signal name="SIO_CLOCKIN">
<contactref element="U$1" pad="AB12"/>
<contactref element="RN4" pad="4"/>
</signal>
<signal name="SIO_CLOCKOUT">
<contactref element="U$1" pad="AA12"/>
<contactref element="RN3" pad="2"/>
</signal>
<signal name="N$99">
<contactref element="R34" pad="2"/>
<contactref element="TR2" pad="B"/>
</signal>
<signal name="N$21">
<contactref element="QS3384" pad="19"/>
<contactref element="RN5" pad="6"/>
<contactref element="S.I.O._INTERFACE" pad="2"/>
</signal>
<signal name="N$100">
<contactref element="QS3384" pad="16"/>
<contactref element="RN5" pad="8"/>
<contactref element="S.I.O._INTERFACE" pad="4"/>
</signal>
<signal name="N$101">
<contactref element="QS3384" pad="15"/>
<contactref element="RN6" pad="6"/>
<contactref element="S.I.O._INTERFACE" pad="6"/>
</signal>
<signal name="N$102">
<contactref element="QS3384" pad="10"/>
<contactref element="RN6" pad="7"/>
<contactref element="S.I.O._INTERFACE" pad="7"/>
</signal>
<signal name="N$103">
<contactref element="QS3384" pad="9"/>
<contactref element="RN6" pad="5"/>
<contactref element="S.I.O._INTERFACE" pad="5"/>
</signal>
<signal name="N$104">
<contactref element="QS3384" pad="6"/>
<contactref element="RN5" pad="7"/>
<contactref element="S.I.O._INTERFACE" pad="3"/>
</signal>
<signal name="N$106">
<contactref element="QS3384" pad="5"/>
<contactref element="RN5" pad="5"/>
<contactref element="S.I.O._INTERFACE" pad="1"/>
</signal>
<signal name="N$108">
<contactref element="D1" pad="1"/>
<contactref element="QS3384" pad="24"/>
<contactref element="C20" pad="1"/>
</signal>
<signal name="N$107">
<contactref element="R33" pad="2"/>
<contactref element="R34" pad="1"/>
<contactref element="QS3384" pad="2"/>
</signal>
<signal name="N$109">
<contactref element="PF3" pad="1"/>
<contactref element="S.I.O._INTERFACE" pad="8"/>
<contactref element="S.I.O._INTERFACE" pad="10"/>
</signal>
<signal name="N$105">
<contactref element="PF3" pad="2"/>
<contactref element="TR2" pad="C"/>
</signal>
<signal name="4V3_INT">
<contactref element="D3" pad="1"/>
<contactref element="IC1" pad="24"/>
<contactref element="C38" pad="1"/>
<contactref element="C39" pad="1"/>
<contactref element="C40" pad="1"/>
<contactref element="C41" pad="1"/>
<contactref element="IC4" pad="24"/>
<contactref element="IC3" pad="24"/>
<contactref element="IC2" pad="24"/>
</signal>
<signal name=".A13">
<contactref element="IC3" pad="23"/>
<contactref element="P.B.I._INTERFACE" pad="34"/>
</signal>
<signal name=".A14">
<contactref element="IC4" pad="2"/>
<contactref element="P.B.I._INTERFACE" pad="35"/>
</signal>
<signal name=".A15">
<contactref element="IC4" pad="5"/>
<contactref element="P.B.I._INTERFACE" pad="36"/>
</signal>
<signal name=".D0">
<contactref element="IC2" pad="2"/>
<contactref element="P.B.I._INTERFACE" pad="13"/>
</signal>
<signal name=".D1">
<contactref element="IC2" pad="6"/>
<contactref element="P.B.I._INTERFACE" pad="15"/>
</signal>
<signal name=".D2">
<contactref element="IC2" pad="10"/>
<contactref element="P.B.I._INTERFACE" pad="17"/>
</signal>
<signal name=".D3">
<contactref element="IC1" pad="23"/>
<contactref element="P.B.I._INTERFACE" pad="10"/>
</signal>
<signal name=".D4">
<contactref element="IC2" pad="20"/>
<contactref element="P.B.I._INTERFACE" pad="21"/>
</signal>
<signal name=".D5">
<contactref element="IC2" pad="16"/>
<contactref element="P.B.I._INTERFACE" pad="19"/>
</signal>
<signal name=".D6">
<contactref element="IC1" pad="20"/>
<contactref element="P.B.I._INTERFACE" pad="9"/>
</signal>
<signal name=".D7">
<contactref element="IC1" pad="19"/>
<contactref element="P.B.I._INTERFACE" pad="8"/>
</signal>
<signal name=".RW_N">
<contactref element="IC1" pad="9"/>
<contactref element="P.B.I._INTERFACE" pad="4"/>
</signal>
<signal name=".REF_N">
<contactref element="IC4" pad="9"/>
<contactref element="R54" pad="2"/>
<contactref element="P.B.I._INTERFACE" pad="38"/>
</signal>
<signal name=".PHI2">
<contactref element="IC1" pad="5"/>
<contactref element="P.B.I._INTERFACE" pad="2"/>
</signal>
<signal name=".MPD_N">
<contactref element="IC4" pad="6"/>
<contactref element="R53" pad="2"/>
<contactref element="P.B.I._INTERFACE" pad="37"/>
</signal>
<signal name=".EXTSEL_N">
<contactref element="IC3" pad="20"/>
<contactref element="R52" pad="2"/>
<contactref element="P.B.I._INTERFACE" pad="33"/>
</signal>
<signal name=".RST_N">
<contactref element="IC4" pad="15"/>
<contactref element="P.B.I._INTERFACE" pad="40"/>
</signal>
<signal name=".IRQ_N">
<contactref element="IC4" pad="10"/>
<contactref element="R55" pad="2"/>
<contactref element="P.B.I._INTERFACE" pad="39"/>
</signal>
<signal name=".CCTL_N">
<contactref element="IC1" pad="2"/>
<contactref element="P.B.I._INTERFACE" pad="1"/>
</signal>
<signal name=".S4_N">
<contactref element="IC3" pad="19"/>
<contactref element="P.B.I._INTERFACE" pad="32"/>
</signal>
<signal name=".S5_N">
<contactref element="IC1" pad="16"/>
<contactref element="P.B.I._INTERFACE" pad="7"/>
</signal>
<signal name=".RD4">
<contactref element="IC3" pad="16"/>
<contactref element="R51" pad="2"/>
<contactref element="P.B.I._INTERFACE" pad="31"/>
</signal>
<signal name=".RD5">
<contactref element="IC1" pad="6"/>
<contactref element="R50" pad="2"/>
<contactref element="P.B.I._INTERFACE" pad="3"/>
</signal>
<signal name=".A10">
<contactref element="IC1" pad="10"/>
<contactref element="P.B.I._INTERFACE" pad="5"/>
</signal>
<signal name=".A11">
<contactref element="IC1" pad="15"/>
<contactref element="P.B.I._INTERFACE" pad="6"/>
</signal>
<signal name=".A12">
<contactref element="IC2" pad="5"/>
<contactref element="P.B.I._INTERFACE" pad="14"/>
</signal>
<signal name=".A9">
<contactref element="IC2" pad="9"/>
<contactref element="P.B.I._INTERFACE" pad="16"/>
</signal>
<signal name=".A8">
<contactref element="IC2" pad="15"/>
<contactref element="P.B.I._INTERFACE" pad="18"/>
</signal>
<signal name=".A7">
<contactref element="IC2" pad="19"/>
<contactref element="P.B.I._INTERFACE" pad="20"/>
</signal>
<signal name=".A6">
<contactref element="IC2" pad="23"/>
<contactref element="P.B.I._INTERFACE" pad="22"/>
</signal>
<signal name=".A0">
<contactref element="IC3" pad="2"/>
<contactref element="P.B.I._INTERFACE" pad="23"/>
</signal>
<signal name=".A5">
<contactref element="IC3" pad="5"/>
<contactref element="P.B.I._INTERFACE" pad="24"/>
</signal>
<signal name=".A1">
<contactref element="IC3" pad="6"/>
<contactref element="P.B.I._INTERFACE" pad="25"/>
</signal>
<signal name=".A4">
<contactref element="IC3" pad="9"/>
<contactref element="P.B.I._INTERFACE" pad="26"/>
</signal>
<signal name=".A2">
<contactref element="IC3" pad="10"/>
<contactref element="P.B.I._INTERFACE" pad="27"/>
</signal>
<signal name=".A3">
<contactref element="IC3" pad="15"/>
<contactref element="P.B.I._INTERFACE" pad="28"/>
</signal>
<signal name="PIO5">
<contactref element="RN30" pad="8"/>
<contactref element="IC1" pad="11"/>
</signal>
<signal name="PIO6">
<contactref element="RN30" pad="7"/>
<contactref element="IC1" pad="14"/>
</signal>
<signal name="PIO7">
<contactref element="RN30" pad="6"/>
<contactref element="IC1" pad="17"/>
</signal>
<signal name="PIO8">
<contactref element="RN30" pad="5"/>
<contactref element="IC1" pad="18"/>
</signal>
<signal name="PIO9">
<contactref element="RN31" pad="8"/>
<contactref element="IC1" pad="21"/>
</signal>
<signal name="PIO10">
<contactref element="RN31" pad="7"/>
<contactref element="IC1" pad="22"/>
</signal>
<signal name="PIO11">
<contactref element="RN31" pad="6"/>
<contactref element="IC2" pad="3"/>
</signal>
<signal name="PIO12">
<contactref element="RN31" pad="5"/>
<contactref element="IC2" pad="4"/>
</signal>
<signal name="PIO4">
<contactref element="RN29" pad="5"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="PIO3">
<contactref element="RN29" pad="6"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="PIO2">
<contactref element="RN29" pad="7"/>
<contactref element="IC1" pad="4"/>
</signal>
<signal name="PIO1">
<contactref element="RN29" pad="8"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="PIO13">
<contactref element="RN32" pad="8"/>
<contactref element="IC2" pad="7"/>
</signal>
<signal name="PIO14">
<contactref element="RN32" pad="7"/>
<contactref element="IC2" pad="8"/>
</signal>
<signal name="PIO15">
<contactref element="RN32" pad="6"/>
<contactref element="IC2" pad="11"/>
</signal>
<signal name="PIO16">
<contactref element="RN32" pad="5"/>
<contactref element="IC2" pad="14"/>
</signal>
<signal name="PIO17">
<contactref element="RN33" pad="8"/>
<contactref element="IC2" pad="17"/>
</signal>
<signal name="PIO18">
<contactref element="RN33" pad="7"/>
<contactref element="IC2" pad="18"/>
</signal>
<signal name="PIO19">
<contactref element="RN33" pad="6"/>
<contactref element="IC2" pad="21"/>
</signal>
<signal name="PIO20">
<contactref element="RN33" pad="5"/>
<contactref element="IC2" pad="22"/>
</signal>
<signal name="PIO21">
<contactref element="RN34" pad="8"/>
<contactref element="IC3" pad="3"/>
</signal>
<signal name="PIO22">
<contactref element="RN34" pad="7"/>
<contactref element="IC3" pad="4"/>
</signal>
<signal name="PIO23">
<contactref element="RN34" pad="6"/>
<contactref element="IC3" pad="7"/>
</signal>
<signal name="PIO24">
<contactref element="RN34" pad="5"/>
<contactref element="IC3" pad="8"/>
</signal>
<signal name="PIO25">
<contactref element="RN35" pad="8"/>
<contactref element="IC3" pad="11"/>
</signal>
<signal name="PIO26">
<contactref element="RN35" pad="7"/>
<contactref element="IC3" pad="14"/>
</signal>
<signal name="PIO27">
<contactref element="RN35" pad="6"/>
<contactref element="IC3" pad="17"/>
</signal>
<signal name="PIO28">
<contactref element="RN35" pad="5"/>
<contactref element="IC3" pad="18"/>
</signal>
<signal name="PIO29">
<contactref element="RN36" pad="8"/>
<contactref element="IC3" pad="21"/>
</signal>
<signal name="PIO30">
<contactref element="RN36" pad="7"/>
<contactref element="IC3" pad="22"/>
</signal>
<signal name="PIO31">
<contactref element="RN36" pad="6"/>
<contactref element="IC4" pad="3"/>
</signal>
<signal name="PIO32">
<contactref element="RN36" pad="5"/>
<contactref element="IC4" pad="4"/>
</signal>
<signal name="PIO33">
<contactref element="RN37" pad="8"/>
<contactref element="IC4" pad="7"/>
</signal>
<signal name="PIO34">
<contactref element="RN37" pad="7"/>
<contactref element="IC4" pad="8"/>
</signal>
<signal name="PIO35">
<contactref element="RN37" pad="6"/>
<contactref element="IC4" pad="11"/>
</signal>
<signal name="PIO36">
<contactref element="RN37" pad="5"/>
<contactref element="IC4" pad="14"/>
</signal>
<signal name="PORTA0">
<contactref element="IC5" pad="2"/>
<contactref element="RN8" pad="4"/>
<contactref element="RN7" pad="5"/>
</signal>
<signal name="PORTA1">
<contactref element="IC5" pad="5"/>
<contactref element="RN8" pad="3"/>
<contactref element="RN7" pad="6"/>
</signal>
<signal name="PORTA2">
<contactref element="IC5" pad="6"/>
<contactref element="RN8" pad="2"/>
<contactref element="RN7" pad="7"/>
</signal>
<signal name="PORTA3">
<contactref element="IC5" pad="9"/>
<contactref element="RN8" pad="1"/>
<contactref element="RN7" pad="8"/>
</signal>
<signal name="PORTA4">
<contactref element="IC5" pad="10"/>
<contactref element="RN9" pad="4"/>
<contactref element="RN10" pad="1"/>
</signal>
<signal name="PORTA5">
<contactref element="IC5" pad="15"/>
<contactref element="RN9" pad="3"/>
<contactref element="RN10" pad="2"/>
</signal>
<signal name="PORTA6">
<contactref element="IC5" pad="16"/>
<contactref element="RN9" pad="2"/>
<contactref element="RN10" pad="3"/>
</signal>
<signal name="PORTA7">
<contactref element="IC5" pad="19"/>
<contactref element="RN9" pad="1"/>
<contactref element="RN10" pad="4"/>
</signal>
<signal name="POT0">
<contactref element="LM339" pad="5"/>
<contactref element="74HCT03" pad="3"/>
<contactref element="RN11" pad="1"/>
<contactref element="C29" pad="1"/>
</signal>
<signal name="POT1">
<contactref element="LM339" pad="7"/>
<contactref element="74HCT03" pad="6"/>
<contactref element="RN11" pad="2"/>
<contactref element="C30" pad="1"/>
</signal>
<signal name="POT2">
<contactref element="LM339" pad="9"/>
<contactref element="74HCT03" pad="8"/>
<contactref element="C32" pad="1"/>
<contactref element="RN11" pad="4"/>
</signal>
<signal name="POT3">
<contactref element="LM339" pad="11"/>
<contactref element="74HCT03" pad="11"/>
<contactref element="C31" pad="1"/>
<contactref element="RN11" pad="3"/>
</signal>
<signal name="TRIG0">
<contactref element="JOY1" pad="6"/>
<contactref element="R43" pad="1"/>
<contactref element="IC5" pad="23"/>
</signal>
<signal name="TRIG1">
<contactref element="JOY2" pad="6"/>
<contactref element="R44" pad="1"/>
<contactref element="IC5" pad="20"/>
</signal>
<signal name="POTIN0">
<contactref element="JOY1" pad="9"/>
<contactref element="RN11" pad="7"/>
</signal>
<signal name="POTIN1">
<contactref element="JOY1" pad="5"/>
<contactref element="RN11" pad="8"/>
</signal>
<signal name="POTIN2">
<contactref element="JOY2" pad="9"/>
<contactref element="RN11" pad="5"/>
</signal>
<signal name="POTIN3">
<contactref element="JOY2" pad="5"/>
<contactref element="RN11" pad="6"/>
</signal>
<signal name="PORTA_PROT0">
<contactref element="JOY1" pad="1"/>
<contactref element="RN8" pad="5"/>
</signal>
<signal name="PORTA_PROT1">
<contactref element="JOY1" pad="2"/>
<contactref element="RN8" pad="6"/>
</signal>
<signal name="PORTA_PROT2">
<contactref element="JOY1" pad="3"/>
<contactref element="RN8" pad="7"/>
</signal>
<signal name="PORTA_PROT3">
<contactref element="JOY1" pad="4"/>
<contactref element="RN8" pad="8"/>
</signal>
<signal name="PORTA_PROT4">
<contactref element="JOY2" pad="1"/>
<contactref element="RN9" pad="5"/>
</signal>
<signal name="PORTA_PROT5">
<contactref element="JOY2" pad="2"/>
<contactref element="RN9" pad="6"/>
</signal>
<signal name="PORTA_PROT6">
<contactref element="JOY2" pad="3"/>
<contactref element="RN9" pad="7"/>
</signal>
<signal name="PORTA_PROT7">
<contactref element="JOY2" pad="4"/>
<contactref element="RN9" pad="8"/>
</signal>
<signal name="4V3_INT1">
<contactref element="D2" pad="1"/>
<contactref element="C28" pad="2"/>
<contactref element="IC5" pad="24"/>
</signal>
<signal name="JIO1">
<contactref element="RN22" pad="8"/>
<contactref element="IC5" pad="3"/>
</signal>
<signal name="JIO2">
<contactref element="RN22" pad="7"/>
<contactref element="IC5" pad="4"/>
</signal>
<signal name="JIO3">
<contactref element="RN22" pad="6"/>
<contactref element="IC5" pad="7"/>
</signal>
<signal name="JIO4">
<contactref element="RN22" pad="5"/>
<contactref element="IC5" pad="8"/>
</signal>
<signal name="JIO5">
<contactref element="RN23" pad="8"/>
<contactref element="IC5" pad="11"/>
</signal>
<signal name="JIO6">
<contactref element="IC5" pad="21"/>
<contactref element="RN23" pad="6"/>
</signal>
<signal name="JIO7">
<contactref element="IC5" pad="22"/>
<contactref element="RN23" pad="7"/>
</signal>
<signal name="JIO8">
<contactref element="RN23" pad="5"/>
<contactref element="IC5" pad="18"/>
</signal>
<signal name="JIO9">
<contactref element="RN24" pad="8"/>
<contactref element="IC5" pad="17"/>
</signal>
<signal name="JIO10">
<contactref element="RN24" pad="7"/>
<contactref element="IC5" pad="14"/>
</signal>
<signal name="N$19">
<contactref element="RN3" pad="8"/>
<contactref element="QS3384" pad="3"/>
</signal>
<signal name="N$64">
<contactref element="RN3" pad="7"/>
<contactref element="QS3384" pad="4"/>
</signal>
<signal name="N$65">
<contactref element="RN3" pad="6"/>
<contactref element="QS3384" pad="7"/>
</signal>
<signal name="N$66">
<contactref element="RN3" pad="5"/>
<contactref element="QS3384" pad="8"/>
</signal>
<signal name="N$67">
<contactref element="RN4" pad="8"/>
<contactref element="QS3384" pad="11"/>
</signal>
<signal name="N$68">
<contactref element="RN4" pad="7"/>
<contactref element="QS3384" pad="18"/>
</signal>
<signal name="N$69">
<contactref element="RN4" pad="6"/>
<contactref element="QS3384" pad="17"/>
</signal>
<signal name="N$70">
<contactref element="RN4" pad="5"/>
<contactref element="QS3384" pad="14"/>
</signal>
<signal name="N$73">
<contactref element="R45" pad="1"/>
<contactref element="R46" pad="2"/>
<contactref element="LM339" pad="4"/>
<contactref element="LM339" pad="6"/>
<contactref element="LM339" pad="8"/>
<contactref element="LM339" pad="10"/>
</signal>
<signal name="N$71">
<contactref element="MAX232" pad="2"/>
<contactref element="C34" pad="1"/>
</signal>
<signal name="N$72">
<contactref element="MAX232" pad="3"/>
<contactref element="C33" pad="2"/>
</signal>
<signal name="N$74">
<contactref element="MAX232" pad="5"/>
<contactref element="C35" pad="2"/>
</signal>
<signal name="N$75">
<contactref element="C33" pad="1"/>
<contactref element="MAX232" pad="1"/>
</signal>
<signal name="N$76">
<contactref element="C35" pad="1"/>
<contactref element="MAX232" pad="4"/>
</signal>
<signal name="N$78">
<contactref element="MAX232" pad="14"/>
<contactref element="X2" pad="2"/>
</signal>
<signal name="N$79">
<contactref element="MAX232" pad="13"/>
<contactref element="X2" pad="3"/>
</signal>
<signal name="N$83">
<contactref element="MAX232" pad="7"/>
<contactref element="X2" pad="8"/>
</signal>
<signal name="N$84">
<contactref element="X3" pad="D+"/>
<contactref element="R30" pad="1"/>
<contactref element="R29" pad="2"/>
<contactref element="USB_A_B" pad="6"/>
</signal>
<signal name="N$87">
<contactref element="X3" pad="D-"/>
<contactref element="R31" pad="2"/>
<contactref element="R32" pad="1"/>
<contactref element="USB_A_B" pad="4"/>
</signal>
<signal name="JIO15">
<contactref element="RN25" pad="6"/>
<contactref element="74HCT03" pad="1"/>
<contactref element="74HCT03" pad="13"/>
<contactref element="74HCT03" pad="2"/>
<contactref element="74HCT03" pad="4"/>
<contactref element="74HCT03" pad="5"/>
<contactref element="74HCT03" pad="9"/>
<contactref element="74HCT03" pad="10"/>
<contactref element="74HCT03" pad="12"/>
</signal>
<signal name="SER1">
<contactref element="RN25" pad="5"/>
<contactref element="MAX232" pad="10"/>
</signal>
<signal name="SER2">
<contactref element="RN26" pad="8"/>
<contactref element="MAX232" pad="11"/>
<contactref element="R47" pad="2"/>
</signal>
<signal name="SER3">
<contactref element="RN26" pad="7"/>
<contactref element="R49" pad="1"/>
</signal>
<signal name="EXP1">
<contactref element="RN26" pad="6"/>
<contactref element="GPIO_B" pad="1"/>
</signal>
<signal name="EXP2">
<contactref element="RN26" pad="5"/>
<contactref element="GPIO_B" pad="2"/>
</signal>
<signal name="EXP3">
<contactref element="RN27" pad="8"/>
<contactref element="GPIO_B" pad="3"/>
</signal>
<signal name="EXP4">
<contactref element="RN27" pad="7"/>
<contactref element="GPIO_B" pad="4"/>
</signal>
<signal name="EXP5">
<contactref element="RN27" pad="6"/>
<contactref element="GPIO_B" pad="5"/>
</signal>
<signal name="EXP6">
<contactref element="RN27" pad="5"/>
<contactref element="GPIO_B" pad="6"/>
</signal>
<signal name="EXP7">
<contactref element="RN28" pad="8"/>
<contactref element="GPIO_B" pad="7"/>
</signal>
<signal name="EXP8">
<contactref element="RN28" pad="7"/>
<contactref element="GPIO_B" pad="8"/>
</signal>
<signal name="EXP9">
<contactref element="RN28" pad="6"/>
<contactref element="GPIO_B" pad="9"/>
</signal>
<signal name="EXP10">
<contactref element="RN28" pad="5"/>
<contactref element="GPIO_B" pad="10"/>
</signal>
<signal name="N$25">
<contactref element="TX" pad="C"/>
<contactref element="R47" pad="1"/>
</signal>
<signal name="N$26">
<contactref element="RX" pad="C"/>
<contactref element="R48" pad="1"/>
</signal>
<signal name="5V00">
<contactref element="PF4" pad="2"/>
<contactref element="JOY2" pad="7"/>
<contactref element="JOY1" pad="7"/>
</signal>
<signal name="JIO11">
<contactref element="RN24" pad="6"/>
<contactref element="RN12" pad="1"/>
<contactref element="LM339" pad="1"/>
</signal>
<signal name="JIO12">
<contactref element="RN24" pad="5"/>
<contactref element="RN12" pad="2"/>
<contactref element="LM339" pad="2"/>
</signal>
<signal name="JIO13">
<contactref element="RN25" pad="8"/>
<contactref element="RN12" pad="3"/>
<contactref element="LM339" pad="14"/>
</signal>
<signal name="JIO14">
<contactref element="RN25" pad="7"/>
<contactref element="RN12" pad="4"/>
<contactref element="LM339" pad="13"/>
</signal>
<signal name="N$63">
<contactref element="R22" pad="1"/>
<contactref element="3V3" pad="A"/>
</signal>
<signal name="N$80">
<contactref element="R23" pad="1"/>
<contactref element="2V5" pad="A"/>
</signal>
<signal name="N$82">
<contactref element="1V1" pad="C"/>
<contactref element="TR1" pad="C"/>
</signal>
<signal name="N$88">
<contactref element="TR1" pad="E"/>
<contactref element="R24" pad="1"/>
</signal>
<signal name="MIC_IN">
<contactref element="ADC" pad="3"/>
<contactref element="MIC_IN_SEL" pad="5"/>
<contactref element="MIC_IN_SEL" pad="1"/>
<contactref element="MIC_IN_SEL" pad="3"/>
</signal>
<signal name="MIC_SIO">
<contactref element="MIC_IN_SEL" pad="4"/>
<contactref element="S.I.O._INTERFACE" pad="9"/>
</signal>
<signal name="MIC_PBI">
<contactref element="MIC_IN_SEL" pad="6"/>
<contactref element="P.B.I._INTERFACE" pad="29"/>
<contactref element="P.B.I._INTERFACE" pad="30"/>
</signal>
<signal name="N$81">
<contactref element="RESET_LED" pad="1"/>
<contactref element="R25A" pad="2"/>
</signal>
<signal name="N$77">
<contactref element="MAX232" pad="6"/>
<contactref element="C36" pad="1"/>
</signal>
<signal name="N$85">
<contactref element="R48" pad="2"/>
<contactref element="MAX232" pad="12"/>
<contactref element="R49" pad="2"/>
</signal>
<signal name="GNDOFF">
</signal>
<signal name=".JIO1">
<contactref element="U$1" pad="F13"/>
<contactref element="RN22" pad="1"/>
</signal>
<signal name=".JIO2">
<contactref element="U$1" pad="G13"/>
<contactref element="RN22" pad="2"/>
</signal>
<signal name=".JIO3">
<contactref element="U$1" pad="A14"/>
<contactref element="RN22" pad="3"/>
</signal>
<signal name=".JIO4">
<contactref element="U$1" pad="E14"/>
<contactref element="RN22" pad="4"/>
</signal>
<signal name=".JIO5">
<contactref element="U$1" pad="F14"/>
<contactref element="RN23" pad="1"/>
</signal>
<signal name=".JIO6">
<contactref element="U$1" pad="H14"/>
<contactref element="RN23" pad="3"/>
</signal>
<signal name=".JIO7">
<contactref element="U$1" pad="A15"/>
<contactref element="RN23" pad="2"/>
</signal>
<signal name=".JIO8">
<contactref element="U$1" pad="B15"/>
<contactref element="RN23" pad="4"/>
</signal>
<signal name=".JIO9">
<contactref element="U$1" pad="G15"/>
<contactref element="RN24" pad="1"/>
</signal>
<signal name=".JIO10">
<contactref element="U$1" pad="E16"/>
<contactref element="RN24" pad="2"/>
</signal>
<signal name=".JIO11">
<contactref element="U$1" pad="D17"/>
<contactref element="RN24" pad="3"/>
</signal>
<signal name=".JIO12">
<contactref element="U$1" pad="G18"/>
<contactref element="RN24" pad="4"/>
</signal>
<signal name=".JIO13">
<contactref element="U$1" pad="H18"/>
<contactref element="RN25" pad="1"/>
</signal>
<signal name=".JIO14">
<contactref element="U$1" pad="J19"/>
<contactref element="RN25" pad="2"/>
</signal>
<signal name=".JIO15">
<contactref element="U$1" pad="K22"/>
<contactref element="RN25" pad="3"/>
</signal>
<signal name=".SER1">
<contactref element="U$1" pad="K19"/>
<contactref element="RN25" pad="4"/>
</signal>
<signal name=".PIO1">
<contactref element="U$1" pad="W16"/>
<contactref element="RN29" pad="1"/>
</signal>
<signal name=".PIO2">
<contactref element="U$1" pad="U16"/>
<contactref element="RN29" pad="2"/>
</signal>
<signal name=".PIO3">
<contactref element="U$1" pad="AB15"/>
<contactref element="RN29" pad="3"/>
</signal>
<signal name=".PIO4">
<contactref element="U$1" pad="AA15"/>
<contactref element="RN29" pad="4"/>
</signal>
<signal name=".PIO25">
<contactref element="U$1" pad="V15"/>
<contactref element="RN35" pad="1"/>
</signal>
<signal name=".PIO26">
<contactref element="U$1" pad="Y15"/>
<contactref element="RN35" pad="2"/>
</signal>
<signal name=".PIO27">
<contactref element="U$1" pad="U15"/>
<contactref element="RN35" pad="3"/>
</signal>
<signal name=".PIO28">
<contactref element="U$1" pad="T15"/>
<contactref element="RN35" pad="4"/>
</signal>
<signal name=".PIO29">
<contactref element="U$1" pad="AA14"/>
<contactref element="RN36" pad="1"/>
</signal>
<signal name=".PIO30">
<contactref element="U$1" pad="V14"/>
<contactref element="RN36" pad="2"/>
</signal>
<signal name=".PIO31">
<contactref element="U$1" pad="Y14"/>
<contactref element="RN36" pad="3"/>
</signal>
<signal name=".PIO32">
<contactref element="U$1" pad="T14"/>
<contactref element="RN36" pad="4"/>
</signal>
<signal name=".PIO33">
<contactref element="U$1" pad="R14"/>
<contactref element="RN37" pad="1"/>
</signal>
<signal name=".PIO34">
<contactref element="U$1" pad="AB13"/>
<contactref element="RN37" pad="2"/>
</signal>
<signal name=".PIO35">
<contactref element="U$1" pad="AA13"/>
<contactref element="RN37" pad="3"/>
</signal>
<signal name=".PIO36">
<contactref element="U$1" pad="V13"/>
<contactref element="RN37" pad="4"/>
</signal>
<signal name=".PIO5">
<contactref element="U$1" pad="P18"/>
<contactref element="RN30" pad="1"/>
</signal>
<signal name=".PIO6">
<contactref element="U$1" pad="P17"/>
<contactref element="RN30" pad="2"/>
</signal>
<signal name=".PIO7">
<contactref element="U$1" pad="R22"/>
<contactref element="RN30" pad="3"/>
</signal>
<signal name=".PIO8">
<contactref element="U$1" pad="R17"/>
<contactref element="RN30" pad="4"/>
</signal>
<signal name=".PIO9">
<contactref element="U$1" pad="T22"/>
<contactref element="RN31" pad="1"/>
</signal>
<signal name=".PIO10">
<contactref element="U$1" pad="T20"/>
<contactref element="RN31" pad="2"/>
</signal>
<signal name=".PIO11">
<contactref element="U$1" pad="T17"/>
<contactref element="RN31" pad="3"/>
</signal>
<signal name=".PIO12">
<contactref element="U$1" pad="U21"/>
<contactref element="RN31" pad="4"/>
</signal>
<signal name=".PIO13">
<contactref element="U$1" pad="V21"/>
<contactref element="RN32" pad="1"/>
</signal>
<signal name=".PIO14">
<contactref element="U$1" pad="V20"/>
<contactref element="RN32" pad="2"/>
</signal>
<signal name=".PIO15">
<contactref element="U$1" pad="W21"/>
<contactref element="RN32" pad="3"/>
</signal>
<signal name=".PIO16">
<contactref element="U$1" pad="Y21"/>
<contactref element="RN32" pad="4"/>
</signal>
<signal name=".PIO17">
<contactref element="U$1" pad="AB22"/>
<contactref element="RN33" pad="1"/>
</signal>
<signal name=".PIO18">
<contactref element="U$1" pad="AB20"/>
<contactref element="RN33" pad="2"/>
</signal>
<signal name=".PIO19">
<contactref element="U$1" pad="Y20"/>
<contactref element="RN33" pad="3"/>
</signal>
<signal name=".PIO20">
<contactref element="U$1" pad="W19"/>
<contactref element="RN33" pad="4"/>
</signal>
<signal name=".PIO21">
<contactref element="U$1" pad="AB18"/>
<contactref element="RN34" pad="1"/>
</signal>
<signal name=".PIO22">
<contactref element="U$1" pad="V18"/>
<contactref element="RN34" pad="2"/>
</signal>
<signal name=".PIO23">
<contactref element="U$1" pad="AA17"/>
<contactref element="RN34" pad="3"/>
</signal>
<signal name=".PIO24">
<contactref element="U$1" pad="Y17"/>
<contactref element="RN34" pad="4"/>
</signal>
<signal name=".SER2">
<contactref element="U$1" pad="K17"/>
<contactref element="RN26" pad="1"/>
</signal>
<signal name=".SER3">
<contactref element="U$1" pad="L22"/>
<contactref element="RN26" pad="2"/>
</signal>
<signal name="GPIOB0">
<contactref element="U$1" pad="E15"/>
<contactref element="RN28" pad="2"/>
</signal>
<signal name="GPIOB1">
<contactref element="U$1" pad="C15"/>
<contactref element="RN28" pad="1"/>
</signal>
<signal name="GPIOB2">
<contactref element="U$1" pad="L18"/>
<contactref element="RN26" pad="3"/>
</signal>
<signal name="GPIOB3">
<contactref element="U$1" pad="M22"/>
<contactref element="RN26" pad="4"/>
</signal>
<signal name="GPIOB4">
<contactref element="U$1" pad="M18"/>
<contactref element="RN27" pad="1"/>
</signal>
<signal name="GPIOB5">
<contactref element="U$1" pad="M16"/>
<contactref element="RN27" pad="2"/>
</signal>
<signal name="GPIOB6">
<contactref element="U$1" pad="N19"/>
<contactref element="RN27" pad="3"/>
</signal>
<signal name="GPIOB7">
<contactref element="U$1" pad="N16"/>
<contactref element="RN27" pad="4"/>
</signal>
<signal name="GPIOB8">
<contactref element="U$1" pad="Y16"/>
<contactref element="RN28" pad="3"/>
</signal>
<signal name="GPIOB9">
<contactref element="U$1" pad="V16"/>
<contactref element="RN28" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
